Heritage Landing Community Development District

Board of Supervisors’ Meeting
December 14, 2023

District Office: 2806 N. Fifth Street Unit 403
St. Augustine, FL 32084 www.heritagelandingcdd.org

HERITAGE LANDING COMMUNITY DEVELOPMENT DISTRICT

Camp Heritage Amenity Center
370 Heritage Landing Parkway, St. Augustine, FL 32092 www.heritagelandingcdd.org

Board of Supervisors	Michael Taylor
Kevin Austin	Chairman
Vice Chairman	
	Robert Och Achara Tarfa Christine Mallatt	Assistant Secretary Assistant Secretary Assistant Secretary	
District Manager	Melissa Dobbins	Rizzetta & Company, Inc.	
District Counsel	Wes Haber	Kutak Rock LLP	
District Engineer	Scott Lockwood	England-Thims & Miller, Inc	

All cellular phones must be placed on mute while in the meeting room.

The Audience Comments portion, on Agenda Items Only, will be held at the beginning of the meeting. The Audience Comments portion of the agenda, on General Items, will be held at the end of the meeting. During these portions of the agenda, audience members may make comments on matters that concern the District (CDD) and will be limited to a total of three (3) minutes to make their comments.

Pursuant to provisions of the Americans with Disabilities Act, any person requiring special accommodations to participate in this meeting/hearing/workshop is asked to advise the District Office at least forty-eight (48) hours before the meeting/hearing/workshop by contacting the District Manager at (239) 936-0913. If you are hearing or speech impaired, please contact the Florida Relay Service by dialing 7-1- 1, or 1-800-955-8771 (TTY)
1-800-955-8770 (Voice), who can aid you in contacting the District Office.

A person who decides to appeal any decision made at the meeting/hearing/workshop with respect to any matter considered at the meeting/hearing/workshop is advised that person will need a record of the proceedings and that accordingly, the person may need to ensure that a verbatim record of the proceedings is made including the testimony and evidence upon which the appeal is to be based.

HERITAGE LANDING COMMUNITY DEVELOPMENT DISTRICT
District Office · St. Augustine, Florida · (904) 436-6270
Mailing Address · 3434 Colwell Avenue, Suite 200, Tampa, Florida 33614 www.heritagelandingcdd.org

Board of Supervisors	December 7, 2023
Heritage Landing Community Development District
AGENDA

Dear Board Members:
The regular meeting of the Board of Supervisors of the Heritage Landing Community Development District will be held on December 14, 2023 at 1:00 p.m. at the Heritage Landing Amenity Center, located at 370 Heritage Landing Parkway, St. Augustine, Florida 32092. The following is the agenda for this meeting:

CALL TO ORDER/ROLL CALL
AUDIENCE COMMENTS ON AGENDA ITEMS
Consent Agenda
Consideration of the Minutes of the Board of Supervisors’
Meeting held on November 9, 2023	Tab 1
Ratification of the Operation and Maintenance Expenditures
for the month of October 2023	Tab 2
STAFF REPORTS - PART A
District Engineer
Landscape and Maintenance	Tab 3
Consideration of BrightView Enhancement Proposal
BUSINESS ITEMS
Consideration of Proposals for RFQ for District Engineer (under separate cover)
Consideration of Proposals for Irrigation Pump Replacement	Tab 4
Consideration of Proposals for Pedestrian Crossing Lighting	Tab 5
STAFF REPORTS - PART B
District Counsel
Amenity Center and Field Maintenance
Amenity Manager Report	Tab 6
Review of Amenity Athletics 2024 Calendar
Review of Chomic Combat Karate Program
Consideration of Vector Security Options
Field Manager Report	Tab 7
Charles Aquatics Report	Tab 8
District Manager
AUDIENCE COMMENTS AND SUPERVISOR REQUESTS
ADJOURNMENT
I look forward to seeing you at the meeting. In the meantime, if you have any questions, please do not hesitate to contact me at (904) 436-6270.

Very truly yours, Melissa Dobbins Melissa Dobbins,

Tab 1

1	MINUTES OF MEETING
2
Each person who decides to appeal any decision made by the Board with respect to
any matter considered at the meeting is advised that the person may need to ensure
that a verbatim record of the proceedings is made, including the testimony and evidence
upon which such appeal is to be based.
7
8
9	HERITAGE LANDING
10	COMMUNITY DEVELOPMENT DISTRICT
11
12	The regular meeting of the Heritage Landing Community Development District was held
13	on Thursday, November 9, 2023, at 6:00 p.m. at the Heritage Landing Amenity Center,
14	located at 370 Heritage Landing Parkway, St. Augustine, Florida 32092.
15
16
17	Present and constituting a quorum:
18
19	Michael Taylor	Board Supervisor, Chairman (speakerphone)
20	Kevin Austin	Board Supervisor, Vice Chairman (joined in progress)
21	Robert Och	Board Supervisor, Assistant Secretary
22	Achara Tarfa	Board Supervisor, Assistant Secretary (speakerphone)
23	Christine Mallatt	Board Supervisor, Assistant Secretary
24
25	Also present were:
26
27	Melissa Dobbins	District Manager, Rizzetta & Company, Inc.
28	Wes Haber	District Counsel, Kutak Rock LLC (speakerphone)
29	Scott Lockwood	District Engineer, England Thims & Miller
30	Lourens Erasmus	General Manager, Vesta Property Services
31	Todd Myhill	Amenity Manager, Vesta Property Services
32	Thomas Rustici	Brightview Landscape
33
34	Public present.
35
36	FIRST ORDER OF BUSINESS	Call to Order
37
38	Mr. Taylor called the meeting to order at 6:00 p.m. and read the roll call.
39
40	SECOND ORDER OF BUSINESS	Public Comments
41
42	No comments.
43
44	THIRD ORDER OF BUSINESS	Consent Items
45
1. Consideration of the Minutes of the Board of Supervisors’
Meeting held October 12, 2023
48
2. Ratification of the Operation and Maintenance Expenditures
for September 2023

On a motion by Mr. Och, seconded by Ms. Mallatt, with all in favor, the Board approved the minutes, of the Meeting held October 12, 2023, and ratified the Operation and Maintenance Expenditures for September 2023 in the amount of $203,622.68, for the Heritage Landing Community Development District.

51

52
53	FOURTH ORDER OF BUSINESS	Consideration of Resolution 2024-01;
54	Amending Fiscal Year 2023 Budget

On a motion by Ms. Mallatt, seconded by Mr. Och, with all in favor, the Board adopted Resolution 2024-01, amending the fiscal year 2023 budget, for the Heritage Landing Community Development District.

55

56
57	Mr. Austin joined the meeting in progress.
58
59	FIFTH ORDER OF BUSINESS	STAFF REPORTS - PART A
60
61	A.	District Engineer
62
Mr. Lockwood presented England Thims & Miller’s 60-day termination letter. The Board
directed the District Manager to proceed with the Request for Qualifications process and
accepted England Thims & Miller’s resignation.
66
Mr. Lockwood noted that he reviewed the area for possible stairs outside the gym to the
geyser area. The Board took no further action on this matter.
69
70	Mr. Lockwood will send final survey for street sign replacement to Mr. Erasmus to then
71	be submitted to the county.
72
73	The Board moved to agenda item 5A.
74
75	SIXTH ORDER OF BUSINESS	Discussion Regarding Amenity
76	Suspensions
77
78	Mr. Myhill updated the Board that all minors have been remorseful and fulfilled their full
79	30-day suspension. He was not going to recommend any further action.
80
81	SEVENTH ORDER OF BUSINESS	STAFF REPORTS – PART B
82
83	B.	Landscape and Maintenance
84
85	1.) Consideration of BrightView Winter Rye Seed Proposal
86
87	After discussion, the Board took no further action.
88
89
90
91

93	EIGHTH ORDER OF BUSINESS	Consideration of Poolsure Renewal
94	Proposal

On a motion by Mr. Taylor, seconded by Mr. Och, with all in favor, the Board approved Poolsure’s 2024 renewal proposal, in the amount of $3,239.00, and to pay in full to receive a 5% discount for the year, for the Heritage Landing Community Development District.

95

96
97	NINTH ORDER OF BUSINESS	Discussion Regarding Survey Plans
98	for Placement of Combo Street
99	Signage & Color Options

On a motion by Mr. Och, seconded by Ms. Mallatt, by majority vote, with Mr. Tarfa opposed, after further discussion the Board approved the taupe color for the poll, white for the cap and street sign background color of white, for the Heritage Landing Community Development District.

100

101
102	TENTH ORDER OF BUSINESS	Staff Reports – PART C
103
104	A.	District Counsel
105
106	No report.
107
108	B.	Amenity Center and Field Maintenance
109
110	1.) Amenity Manager Report
111
112	i.	Hammerhead Swim Team Polar Plunge Event
113
After discussion, the Board authorized Ms. Mallatt to work with Mr. Myhill to review details
of the event, subject to the District Manager confirming if there is any additional insurance
required for Lifeguards to be hired on a volunteer basis by the swim team.
117
118	ii.	Request to Use District Tennis Courts
119
After discussion, the board advised that this event get reviewed again after dates have
been confirmed for when the courts are going to be resurfaced for pickle ball.
122
Mr. Myhill stated he will also do the same and confirm dates with the new tennis instructor
on when they can use the courts.
125
126	Mr. Erasmus’ further stated that the resurfacing will need to wait until Spring since the
127	warmer weather will be the right time for the contractor to use their specific product for this
128	project, especially if it’s going to be done the “right way”.
129
130	2.) Field Manager Report
131
132	Mr. Erasmus reported that conduit is being laid down for the lighting of the medians and
133	the well install contractor’s deposit was paid.

135
136
137	i.	Discussion Regarding Dock & Bridge Proposal
138
139	It was stated that more information on the dock and bridge should hold off until a new
140	District Engineer is hired to get their feedback as this matter.
141
142	3.) Charles Aquatics Pond Report
143
144	The Board requested an update on when the next carp install will occur, for which ponds
145	and how many.
146
147	C.	District Manager
148
Ms. Dobbins updated the Board that the full amount of $140,000.00 donation for the street
signs and the pickleball courts was received today by the HOA.
151
Ms. Dobbins confirmed with the Board that the Staff can use the $2,000.00 gift card for
supplies and repairs that UPS paid the District for the Holiday POD.
154
155 ELEVENTH ORDER OF BUSINESS	Supervisor Requests and Audience
156	Comments
157
158	Supervisors:
159
160	No comments.
161
162	Audience:
163
164	No comments.
165
166	TWELFTH ORDER OF BUSINESS	Adjournment
167
On a motion by Mr. Taylor, seconded by Mr. Och with all in favor, the Board adjourned the meeting at 7:29 p.m., for the Heritage Landing Community Development District.
168
169
170
171
172
173
174
175
176
177
178
179
180

182		
183		
184		
185		
186		
187		
188		
189		
190	 		
191	Secretary/Assistant Secretary	
192		
193		
194		
195		
196		

 	
Chairman/Vice Chairman

Tab 2

HERITAGE LANDING COMMUNITY DEVELOPMENT DISTRICT

DISTRICT OFFICE · ST. AUGUSTINE, FLORIDA 32084
Mailing Address · 3434 Colwell Avenue, Suite 200 · Tampa, Florida 33614 Www.HeritageLandingCdd.Org

Operation and Maintenance Expenditures
October 2023 Presented For Board Approval

Attached please find the check register listing the Operation and Maintenance expenditures paid from October 1, 2023 through October 31, 2023. This does not include expenditures previously approved by the Board.

The total items being presented:    $119,083.52

Approval of Expenditures:

	 Chairperson

	 Vice Chairperson

	 Assistant Secretary

Paid Operation & Maintenance Expenditures	
October 1, 2023 Through October 31, 2023	

Vendor Name		
Check Number Invoice Number		
Invoice Description		
Invoice Amount	
All Weather Contractors, Inc.	100431	168327	Water Park Repairs 09/23	$	1,990.00	
BrightView Landscape Services, Inc.
BrightView Landscape Services, Inc.
BrightView Landscape Services, Inc.
BrightView Landscape Services, Inc.
BrightView Landscape Services, Inc.
BrightView Landscape Services, Inc.
BrightView Landscape Services, Inc.
BrightView Landscape Services, Inc.
Charles Aquatics, Inc.	100408

100409

100413

100414

100422

100423

100424

100432

100433	8605773

8605745

8595991

8629565

8635678

8635679

8635666

8614220

49131	Debris Removal 09/23 Electrical Repairs 09/23 Irrigation Repairs 09/23 Tree Maintenance 09/23 Irrigation Repairs 10/23 Irrigation Repairs 10/23 Irrigation Repairs 10/23
Landscape Maintenance 10/23

Pond Maintenance 10/23	$

$

$

$

$

$

$

$

$	495.00

2,382.95

604.01

857.40

1,160.70

3,319.78

1,179.60

21,424.00

975.00	
Christine Mallatt	100425	CM101223	Board of Supervisors Meeting 10/12/23	$	200.00	
COMCAST	ACH	8495 74 140 0429787
09/23	Cable TV & Internet 09/23	$	546.46	

Vendor Name	 Check Number Invoice Number	 Invoice Description	 Invoice Amount

England, Thims & Miller, Inc.	100426	210295	Engineering Services 09/23	$	512.50	
Florida Department of Revenue	100415	65-8015563124-2 Sales
& Use Tax 09/23	65-8015563124-2 Sales & Use Tax 09/23	$	439.86	
Florida Power & Light Company	ACH	87098-35048 09/23	Electric Services 09/23	$	4,447.04	
Florida Power & Light Company	ACH	Monthly Summary 09//23	Electric Services 09/23	$	4,411.40	
Heritage Landing CDD			Debit Card Replenishment 10/23	$	1,903.57	
Investment Painting of North FL, LLC	100419	3505	Exterior Painting 10/23	$	1,500.00	
Kevin Lee Austin	100427	KA101223	Board of Supervisors Meeting 10/12/23	$	200.00	
Kutak Rock, LLP	100416	3292418	Legal Services 08/23	$	1,975.50	
Kutak Rock, LLP	100434	3295950	Legal Services - Interpleader Litigation 10/23	$	10,000.00	
Leslie Achara McNair-Tarfa	100428	AT101223	Board of Supervisors Meeting 10/12/23	$	200.00	
Michael C. Taylor	100429	MT101223	Board of Supervisors Meeting 10/12/23	$	200.00	
Northeast Quality Services LLC	100437	32568	Janitorial Services 10/23	$	700.00	

Vendor Name		Check Number Invoice Number		Invoice Description		Invoice Amount	
Northeast Quality Services LLC	100438	32273	Janitorial Services 09/23	$	900.00	
Poolsure	100435	131295617811	Pool Chemicals 10/23	$	2,999.63	
Rizzetta & Company, Inc.	100406	INV0000084054	Assessment Roll 10/23	$	5,000.00	
Rizzetta & Company, Inc.	100407	INV0000084151	District Management Fees 10/23	$	5,900.00	
Rizzetta & Company, Inc.	100421	INV0000084337	Public Records Requests 10/23	$	20.00	
Robert Och	100430	RO101223	Board of Supervisors Meeting 10/12/23	$	200.00	
St Johns Utility Department	ACH	503699-115198 09/23	Water Services 09/23	$	1,068.67	
Synergy Florida	100410	375556	Service Call - Audio & Video System	$	218.90	
			09/23			
Treeco	100411	9647	Tree Maintenance 09/23	$	2,900.00	
Turner Pest Control, LLC	100412	617706986	Pest Control Services 09/23	$	127.34	
Vector Security, Inc	100420	72773103	Security Monitoring Services 09/23	$	139.00	

Vendor Name	 Check Number Invoice Number	 Invoice Description	 Invoice Amount

Vesta Property Services, Inc.	100417	414050	Management Services 09/23	$	37,047.66	
Vesta Property Services, Inc.	100418	414163	Reimbursable Expenses 09/23	$	328.04	
VGlobal Tech	100436	5505	ADA Website Maintenance 10/23	$	250.00	
Waste Management Inc. of Florida	ACH	0035107-4032-1	Waste Disposal Service 10/23	 $	359.51	

Report Total	 $	119,083.52

Tab 3

Quality Site Assessment
Prepared for: Heritage Landing @ WGV

General Information

DATE:	Tuesday, Dec 05, 2023	
NEXT QSA DATE:	Monday, Mar 04, 2024	
CLIENT ATTENDEES:	Lourens Erasmus	
BRIGHTVIEW ATTENDEES:	Thomas Rustici	

Customer Focus Areas

Turf health, Annuals, Weed control, Plant Health

Carryover Items

 1 

 2 

 1 

There are some vines and weeds growing in loropetalum Edge between athletic field and clubhouse. We will get with our team and have this addressed.

 2 

There are some vines and volunteers growing up through Jasmine at center island before clubhouse. We will get these hand pulled and schedule an over the top selective to be treated in Jasmine beds to help with weed control.

 1 

The detail work at the clubhouse and pool area looks good and maintained.

 2 

We continue to cut the Ornamental grasses back throughout the community.

 3 

The flowers at the main entrance still look good.

 4 

The turf color through the community still looks good for this time of year.

 4 

 3 

Maintenance Items

 1 

 2 

Maintenance Items

 5 

 5 

We did notice an area of Fungus in the back athletic field. Agrow pro has been notified. We will monitor the area and follow up.

Recommendations for Property Enhancements

 1 

 1 

We would recommend removing/replacing the Roses and Society Garlic from the areas and install some new plants. We will send a proposal.

Notes to Owner / Client

 1 

 2 

 1 

It has been noted that the irrigation is running too much on the turf areas near the RV storage area. This will be adjusted.

 2 

BrightView has installed new sod in some of the bad areas along Heritage Landing Dr. Free of charge.

 1 

Hard and soft surfaces are being sprayed for weed control on a weekly rotation

 2 

There are some fallen debris from previous storm on the ground by dugout. We will get this cleaned up during next visit.

 3 

There are a few tree suckers pushing out in select areas by amenities. We will get with our team and have these removed during their next rotations.

 4 

Plant material is being trimmed on a weekly rotation

 4 

 3 

Completed Items

 1 

 2 

Completed Items		
 5 	 6 			
		 5 	Turf color is starting to improve. A fertilizer,	
			pre-emergent, and	
			insecticide application	
			was applied in April.	
		 6 	The spring flower change out has been installed it	
			and are looking vibrant	
		 7 	
Colgon grass areas have been retreated. We will	
			do a follow up treatment	
 7 	 8 		in a few weeks.	
		 8 	Lakes are being mowed on a weekly rotation	

 9 

Woodline encroaching by Silver Glen and flowers intersection needs to be trimmed back away from sidewalk. We will follow up once completed.

10

Hard and soft surfaces are being edged on a weekly rotation

11

Turf color is starting to improve

12

Annuals are holding up. some of the celosia have mites, we have scheduled a treatment this week while on site

12

11

Completed Items

 9 

10

13

There are some fall out structures throughout the property along preserves that are overgrown, I will get with our team to have these weedeated and sprayed out. We will follow up once completed.

14

Crepe myrtle suckers were removed at crosswalk this week while on site.

15

Shrubs are being trimmed on a weekly rotation

16

Hard and soft surfaces are being sprayed for weed control on a weekly rotation

16

15

Completed Items

13

14

Completed Items

17

17

Remaining 4 flower pots inside pool area have been installed

Proposal for Extra Work at Heritage Landing @ WGV	

Property Name Property Address	
Heritage Landing @ WGV 370 Heritage Landing Pkwy Saint Augustine, FL 32092	
Contact To
Billing Address	
Lourens Erasmus Heritage Landing CDD
c/o Rizzetta and Company Inc 370
Heritage Landing Pkwy St Augustine, FL 32092	
Project Name Project Description	Heritage Landing- Clubhouse plant install enhancement
Scope of Work	

QTY	
UoM/Size	
Material/Description	
Total	

Plant and sod	install		$10,824.19	

1.00	
LUMP SUM	Mobilization and labor to resize beds as needed, rough grade areas as needed, and remove and dispose of		
		waste.		
30.00	EACH	Podocarpus- 7 gal plants installed		
30.00	EACH	Azalea- 3 gal plants installed		
4.00	EACH	Hawaiian Thai- 3 gal plants installed		
20.00	EACH	croton- 3 gal plants installed		
48.00	EACH	Blue daze- 1 gal plants installed		
25.00	EACH	Foxtail fern- 1 gal plants installed		
18.00	EACH	Fakahatchee- 3 gal plants installed		
3.00	EACH	Pygmy date palm - 30 gal installed		
75.00	BAG	gold mulch		
1.00	LUMP SUM	plant delivery fee		
1.00	LUMP SUM	Irrigation modifications and adjustments		
Sable Palm Optioin	$1,584.44	

2.00	
EACH	
Sable palm- installed per tree		
2.00	EACH	tree stake kit		
6.00	EACH	2x4 bracing		
2.00	EACH	box of 2 3/4" screws to secure bracing		
Magnolia Tree			$245.47	
1.00	EACH	Magnolia little Gem-15 gal installed per tree		
1.00	EACH	tree stake kit installed		
Annuals			$675.84	
300.00	EACH	Annuals installed in 4 beds		

Images

Blue-Daze-4	croton mammy

Pygmy Date Palm	Fashion Azalea

dwarf bottle brush	oleander

Liriope

Other
cordyline fruticosa	Foxtail fern

Podocarpus-Pringles-Dwf2	Podocarpus

For internal use only			
SO#	8297887		
JOB#	460802023			
Service Line	130	Total Price	$13,329.94	

TERMS & CONDITIONS

I. The Contractor shall recognize and perform in accordance with written terms, written specifications and drawings only contained or referred to herein. All materials shall conform to bid specifications.

Work Force: Contractor shall designate a qualified representative with experience in landscape rraintenance/construction upgrades or when applicable in tree management. The vYOrkforce shall be competent and qualified, and shall be legally authorized to work in the U.S.

License and Permits: Contractor shall maintain a Landscape Contractor's license, if required by State or local law, and will con-ply with all other license requirements of the City, State and Federal Governments, as we 11 as all other requirements of law. Unless otherwise agreed upon by the parties or prohibited by law, Custorrer shall be required to obtain all necessary and required permits to allow the conmencement of the Services on the property.

Taxes: Contractor agrees to pay all applicable taxes, including sales or General Excise Tax (GET], where applicable.

	Insurance: Contractor agrees to provide General Liability Insu ranee, Automotive Liability Insurance, Worker's Corrpensation Insurance, and any other insurance required by law or Custorrer, as specffied in writing prior to commencerrent of work. If not specified, Contractor will furnish insurance with $1,000.(IDlimit of liability.

Liability: Contractor shall not be liable for any damage that occurs from Acts of God defined as extreme weather conditions, fire, earthquake, etc. and rules, regulations or restrictions irrposed by arry governrrent or governmental agency, national or regional emergency, epidemic, pandemic, health related outbreak or other medical events not caused by one or other delays or failure of perforrrance beyond the conmercially reasonable control of either party. Under these circurrstances, Cortractor shall have the right to renegotiate the terms and prices of this Contract within sixty (60) days.

	Any illegal trespass, claims and/or damages resulting from work requested that is not on property owned by Customer or not under Customer rranagement and control shall be the sole responsibility of the Customer.
s. Subcontractors: Contractor reserves the right to hire qualified subcontractors to perform specialized functions or work requiring specialized equipment.

	Additional Services: Any additional work not shown in the above specifications involving extra costs will be executed only upon signed written orders, and will become an extra charge over and above the estimate.

	Cancellation: Notice of Cancellation of work rrust be received in writing before the crew is dispatched to their location or Customer will be liable for a minimum travel charge of 5150.00 and billed to Customer.

The following sections shall apply where Contractor provides Customer with tree care services:

Tree & Sturr() Rem:>val: Trees removed will be cut as close to the ground as possible based on conditions to or next to the bottom of the tree trunk. Additional charges will be levied for unseen hazards such as, but not linited to concrete brick filled trunks, metal rods, etc. If requested mechanical grinding of visible tree stump will be done to a defined width and depth below ground level at an additional charge to the Customer. Defined backfill and landscape material may be specified. Customer shall be responsible for contacting the appropriate underground utility locator company to locate and mark underground utility lines prior to start of work Contractor is not responsible damage done to underground utilities su::h as but not limited to, cables, wires, pipes, and irrigation parts. Contractor will repair damaged irrigation lines at the Customer's expense.

Waiver of Liability: Requests for crown thinning in excess of twenty-five percent (25%) or work not in accordarce with ISA (international Society of Arboricultural) standards will require a signed waiver of liability.

Acceptance of this Contract
By executing this documenl Customer agrees to the formation of a binding contract and to the terms and conditions set forth herein. Customer represents that Contractor is authorized to perform the ¼'Ork stated on the face of this Contract. If payment has not been received by Contractor per payment terms hereunder, Contractor shall be entitled to all costs of collection, including reasonable attorneys' fees and it shall be relieved of any obligation to continue performance under this or arry other Cortract with Custorrer. Interest at a per annum rate of
1.5% per month (18% per year), or the highest rate permitted D/ law, may be charged on unpaid balance 15 days after billing.

NOTICE: FAILURE TO MAKE PAYMENT WHEN DUE FOR COMPLETED WORK ON CONSTRUCTION JOBS, MAY RESULT IN A MECHANIC'S LIEN ON THE TITLE TO YOUR PROPERTY

Customer

	Access to ..k>bsite: Customer shall provide all utilities to perform the work Customer shall furnish access to all parts of jobsite where Contractor is to perform work as required by the Contract or other functions re 1 ate d thereto, during normal business hours and other reasonable periods of time. Contractor will perform the work as reasonably practical after the Customer makes the site available for performance of the work.

Payment Terms: Upon signing this Agreement, Customer shall pay Contractor 50% of the Proposed Price and the remaining balance shall be paid by Customer to Contractor upon completion of the project unless otherwise, agreed to in writing.

Signature

Lourens Erasmus
Printed Name

Title

Date

Property Manager

December 07, 2023

Termination: This Work Order rray be terrrinated by the either party with or without cause, upon seven (7) workdays advance written notice. Customer will be required to pay for all rraterials purchased and work corr()lete to the date of termination and reasonable charges incurred in dem:>bilizing.

	Assignment: The Customer and the Contractor respectively, bind themselves, their partners, successors, assignees and legal represertatlve to the other party with respect to all covenants of this Agreement. Neither the Custorrer nor the Contractor shall assign or transfer any interest in this Agreerrent without the written consent of the other provided, however, that consent shall not be required to assign this Agreement to any corrpany which controls, is controlled by, or is under comnon control with Contractor or in connection with assignment to an affiliate or pursuant to a merger, sale of all or substartially all of its assets or equity securities, consolidation, change of control or

BrightView Landscape Services, Inc. "Contractor''
Account Manager
Signature	Title

Steve McAvoy	December 07, 2023

Printed Name	Date

corporate reorganization.

Disclaimer: This proposal was estimated and priced based UJX>n a site visit and visual inspection from ground level using ordinary means, at or about the time this proposal was prepared The price quoted in this proposal f o r the work described, is the result of that ground level visual inspection and therefore our corrpany will not be liable for any additional costs or damages for additional ¼'Ork not described herein, or liable for any incidents/accidents resulting from conditions, that were not ascertainable by said ground
level visual inspection bf ordinary means at the time said inspection was performed.
Contractor cannot be held responsible for unknown or otherwise hidden defects. Any corrective work proposed herein cannot guarantee exact results. Professional engineering, architectural, and/or landscape design services ("Design Services') are not ircluded in this Agreement and shall not be provided by the Contractor. Any design defects in the Contract Documents are the sole responsibility of the Customer. If the Customer must engage a licensed engineer, architect and/or landscape design professional, any costs concerning these Design Services are to be paid by the Customer direct to the designer involved.

Job#: SO#:

460802023
8297887

Proposed Price:	$13,329.94

Blue Daze

Annuals

Podocarpus Pygmy Date Palm

Azalea

Foxtail Fern

Crotons

Sable Palm Option

Hawaiian Thai

Option 2

Arboricola	Emerald Goddess Liriope

Tab 4

HERITAGE LANDING CDD	
PROPOSAL WORKSHEET	
JOB	QTY	VENDOR	QUOTE	NOTES	ACTION	
Steamboat irrigation pump						
replacement		BrightView	$16,800			
		Partridge	$11,800			
Install VFD on the irrigation
system		
BrightView	
$23,965			
		
Partridge	
$10,200	If we do it at the same time as the pump
install it would be $8,500		

Wiring the VFD on to system		

Under Separate Cover	

$4,500	
Over the phone guestimate is not more than $4,500 to complete the wiring.		

12/6/23, 10:53 AM	Mail - Lourens Erasmus - Outlook

Heritage Landing- Costly repairs

Good afternoon, Lourens.

I understand your frustration with the costly irrigation repairs we are facing at Heritage Landing. The main focus for me would be the mainline breaks that we continue to repair month to month. The system has been in the ground 20+ years and the schedule 40 fittings continue to fail from water hammer. I sent out a proposal to install a VFD “Variable Flow Drive” to ease the impact but the board decided to go in a different direction with a Nelson Pilot valve. The VFD slows the pump down while the nelson valve slows the water downstream of the unit itself. We tried to sway them away from this in the board meeting at that time as we’re not comfortable using something we have no experience with. (We’ve had great success with the VFD on properties around your age as we don’t run into a mainline break nearly as many times as we do in Heritage. In fact, 90% less would be an understatement) So far the Nelson valve has yielded little to no results. As we keep running into the same issue (Mainline breaks every month). The VFD won’t repair the damage that has already set in but it we’ll ease the amount of further damage caused by not having the mechanism in place to stop the pump from coming on full tilt upon every pressure drop. With different size zones throughout the property the VFD can regulate pressure to our desired amount depending what’s running. We can’t regulate the amount of flex hose blowouts, leaking heads, not rotating heads, clogged nozzles, failed valves or wiring issues that come about but this is the first step to saving money on a monthly 1,000.00+ expense before we even start the inspection.

Juwan Dupree Irrigation Manager

https://outlook.office.com/mail/id/AAQkADY0OWNmNmJjLTQzYjctNDA4Ny04ZTA5LTEyNDU1YTVhM2QxYwAQAKeBVAwCsRlCn6Vlq2VG7UQ%3D	1/1

Proposal for Extra Work at Heritage Landing @ WGV	

Property Name Property Address	
Heritage Landing @ WGV 370 Heritage Landing Pkwy Saint Augustine, FL 32092	
Contact To
Billing Address	
Lourens Erasmus Heritage Landing CDD
c/o Rizzetta and Company Inc 370
Heritage Landing Pkwy St Augustine, FL 32092	
Project Name	Heritage Landing: 20hp motor replacement, motor starter and pressure tank	
Project Description	Heritage Landing: 20hp motor replacement, motor starter and pressure tank
Scope of Work	

QTY

1.00	
UoM/Size

LUMP SUM	
Material/Description
20HP 230v 3ph motor starter with 230v coil FL-30 tank and PJR-6 tank gauges 1.25" psi relief valve parts and labor	
Unit Price

$16,800.00	
Total

$16,800.00	

For internal use only			
SO#	8291824		
JOB#	460802023			
Service Line	150	Total Price	$16,800.00	
THIS IS NOT AN INVOICE
This proposal is valid for thirty (30) days unless otherwise approved by Contractor's Senior Vice President
5811 County Rd 305, Elkton, FL 32033 ph. fax

TERMS & CONDITIONS

I. The Contractor shall recognize and perform in accordance with written terms, written specifications and drawings only contained or referred to herein. All materials shall conform to bid specifications.

Work Force: Contractor shall designate a qualified representative with experience in landscape rraintenance/construction upgrades or when applicable in tree management. The vYOrkforce shall be competent and qualified, and shall be legally authorized to work in the U.S.

License and Permits: Contractor shall maintain a Landscape Contractor's license, if required by State or local law, and will con-ply with all other license requirements of the City, State and Federal Governments, as we 11 as all other requirements of law. Unless otherwise agreed upon by the parties or prohibited by law, Custorrer shall be required to obtain all necessary and required permits to allow the conmencement of the Services on the property.

Taxes: Contractor agrees to pay all applicable taxes, including sales or General Excise Tax (GET], where applicable.

	Insurance: Contractor agrees to provide General Liability Insu ranee, Automotive Liability Insurance, Worker's Corrpensation Insurance, and any other insurance required by law or Custorrer, as specffied in writing prior to commencerrent of work. If not specified, Contractor will furnish insurance with $1,000.(IDlimit of liability.

Liability: Contractor shall not be liable for any damage that occurs from Acts of God defined as extreme weather conditions, fire, earthquake, etc. and rules, regulations or restrictions irrposed by arry governrrent or governmental agency, national or regional emergency, epidemic, pandemic, health related outbreak or other medical events not caused by one or other delays or failure of perforrrance beyond the conmercially reasonable control of either party. Under these circurrstances, Cortractor shall have the right to renegotiate the terms and prices of this Contract within sixty (60) days.

	Any illegal trespass, claims and/or damages resulting from work requested that is not on property owned by Customer or not under Customer rranagement and control shall be the sole responsibility of the Customer.
s. Subcontractors: Contractor reserves the right to hire qualified subcontractors to perform specialized functions or work requiring specialized equipment.

	Additional Services: Any additional work not shown in the above specifications involving extra costs will be executed only upon signed written orders, and will become an extra charge over and above the estimate.

	Cancellation: Notice of Cancellation of work rrust be received in writing before the crew is dispatched to their location or Customer will be liable for a minimum travel charge of 5150.00 and billed to Customer.

The following sections shall apply where Contractor provides Customer with tree care services:

Tree & Sturr() Rem:>val: Trees removed will be cut as close to the ground as possible based on conditions to or next to the bottom of the tree trunk. Additional charges will be levied for unseen hazards such as, but not linited to concrete brick filled trunks, metal rods, etc. If requested mechanical grinding of visible tree stump will be done to a defined width and depth below ground level at an additional charge to the Customer. Defined backfill and landscape material may be specified. Customer shall be responsible for contacting the appropriate underground utility locator company to locate and mark underground utility lines prior to start of work Contractor is not responsible damage done to underground utilities su::h as but not limited to, cables, wires, pipes, and irrigation parts. Contractor will repair damaged irrigation lines at the Customer's expense.

Waiver of Liability: Requests for crown thinning in excess of twenty-five percent (25%) or work not in accordarce with ISA (international Society of Arboricultural) standards will require a signed waiver of liability.

Acceptance of this Contract
By executing this documenl Customer agrees to the formation of a binding contract and to the terms and conditions set forth herein. Customer represents that Contractor is authorized to perform the ¼'Ork stated on the face of this Contract. If payment has not been received by Contractor per payment terms hereunder, Contractor shall be entitled to all costs of collection, including reasonable attorneys' fees and it shall be relieved of any obligation to continue performance under this or arry other Cortract with Custorrer. Interest at a per annum rate of
1.5% per month (18% per year), or the highest rate permitted D/ law, may be charged on unpaid balance 15 days after billing.

NOTICE: FAILURE TO MAKE PAYMENT WHEN DUE FOR COMPLETED WORK ON CONSTRUCTION JOBS, MAY RESULT IN A MECHANIC'S LIEN ON THE TITLE TO YOUR PROPERTY

Customer

	Access to ..k>bsite: Customer shall provide all utilities to perform the work Customer shall furnish access to all parts of jobsite where Contractor is to perform work as required by the Contract or other functions re 1 ate d thereto, during normal business hours and other reasonable periods of time. Contractor will perform the work as reasonably practical after the Customer makes the site available for performance of the work.

Payment Terms: Upon signing this Agreement, Customer shall pay Contractor 50% of the Proposed Price and the remaining balance shall be paid by Customer to Contractor upon completion of the project unless otherwise, agreed to in writing.

Signature

Lourens Erasmus
Printed Name

Title

Date

Property Manager

November 29, 2023

Termination: This Work Order rray be terrrinated by the either party with or without cause, upon seven (7) workdays advance written notice. Customer will be required to pay for all rraterials purchased and work corr()lete to the date of termination and reasonable charges

BrightView Landscape Services, Inc. "Contractor"
Irrigation Manager

incurred in dem:>bilizing.

	Assignment: The Customer and the Contractor respectively, bind themselves, their partners, successors, assignees and legal represertatlve to the other party with respect to all covenants of this Agreement. Neither the Custorrer nor the Contractor shall assign

Signature

Juwan Lamar Dupree

Title

November 29, 2023

or transfer any interest in this Agreerrent without the written consent of the other provided, however, that consent shall not be required to assign this Agreement to any corrpany which controls, is controlled by, or is under comnon control with Contractor or in connection with assignment to an affiliate or pursuant to a merger, sale of all or substartially all of its assets or equity securities, consolidation, change of control or corporate reorganization.

Disclaimer: This proposal was estimated and priced based UJX>n a site visit and visual inspection from ground level using ordinary means, at or about the time this proposal was prepared The price quoted in this proposal f o r the work described, is the result of that ground level visual inspection and therefore our corrpany will not be liable for any additional costs or damages for additional ¼'Ork not described herein, or liable for any incidents/accidents resulting from conditions, that were not ascertainable by said ground
level visual inspection bf ordinary means at the time said inspection was performed.
Contractor cannot be held responsible for unknown or otherwise hidden defects. Any corrective work proposed herein cannot guarantee exact results. Professional engineering, architectural, and/or landscape design services ("Design Services') are not ircluded in this Agreement and shall not be provided by the Contractor. Any design defects in the Contract Documents are the sole responsibility of the Customer. If the Customer must engage a licensed engineer, architect and/or landscape design professional, any costs concerning these Design Services are to be paid by the Customer direct to the designer involved.

Printed Name	Date

Job#:	460802023		
SO#:	8291824	Proposed Price: $16,800.00	

Partridge Well Drilling	Rep	R Stevens	Date 11/30/2023  Contract #	45329
4744 Collins Road	Rep	Valid through 12/30/2023 Customer #	38533 Jacksonville, FL 32244
Phone (904) 269-1333	(904) 355-3323
Established 1892
Vesta Property Services 200 Business Park Cir Suite 101
St Augustine, FL 32095
Site	Heritage Landing	Site # 37109	Contact
Office
Other	Lourens Erasmus	Primary
Home Cell			
	904-940-6095				
			904-536-6217		
Heritage Landing Pkwy St Augustine , FL 32092	County	St Johns

 Replace existing 20HP 230 volt 3 phase submersible pump motor,	

 starter with 230 volt coil, FL-30 tank, PRJ-6 tank, 1.25" PSI relief	

valve, and pressure gauge.

1	$11,800.00	$11,800.00

Condition of well is unknown.

If well is damaged or if the existing pump is stuck in well, there would be additional charges.

Price assumes we can easily access the well head with our hoist truck and there are no obstructions or electrical wires overhead.

While the pump is being removed and reinstalled the artesian well will flow uncontrolled. Mitigation of the uncontrolled flow is not included in this quote.

Price does not include any parts not listed in this quote.

Adding a VFD would be an additional $8,500.00 at the time this work was done. It would be approximately $1,700.00 more to do in the future. If a VFD is installed now, the starter will not be needed. An electrician would be required to wire the VFD and that is not included in this price.

Service Rates	1 Man	$210.00	Additional Hour	$160.00

**PRICE SUBJECT TO CHANGE UPON SITE EVALUATION AND PERMITTING**

Total	$11,800.00

A 50% deposit of $5,900.00 is required. $	 Received on 	/	/	
THE BALANCE FOR EACH ITEM WILL BE DUE WHEN INVOICED. A service charge of 1.5% per month will be charged on past due accounts. Unless Buyer notifies Seller in writing within fifteen (15) days from date of invoice, it shall be presumed that goods and services are satisfactory and acceptable to Buyer. Buyer shall pay Seller's cost of collection including a reasonable attorney's fee at all levels of court. Owners Grant to Partridge Well Co., Inc. the right to enter upon and drive vehicles including heavy trucks, over his property to site using most efficient means of ingress and egress at sole discretion of Partridge Well Co., Inc. and agrees to release and save harmless Partridge Well Co., Inc. from any and all damage to said property and all equipment, fixtures or improvements located upon, on or under the ground. This proposal is subject to change unless signed, returned and order to proceed is given within 30 days. The above proposal is accepted at the prices and terms specified herein. It is agreed that the seller will retain title to any equipment or materials that may be furnished until final payment is made as agreed. The seller shall have rights to remove same and seller will be held harmless for any damages resulting from the removal thereof. This contract voids previous contract(s) with the same contract number. It is the owner’s responsibility to identify and mark the location of any and all private utilities including but not limited to cables, wires, pipes, gas lines, septic tanks and drainfields etc. Owners agree to release and hold harmless Partridge Well Drilling Co. Inc. from any and all damages to said private utilities.

	/	/			

11/30/2023

Signature Owner/ Contractor	Print Name	Date	PWD Representative	Date
	 			/	/	 Signature Owner/ Contractor		Print Name	Date

Contract #	45329	Page 1 of 1

Proposal for Extra Work at Heritage Landing @ WGV

Property Name	Heritage Landing @ WGV	Contact	Lourens Erasmus Property Address	370 Heritage Landing Pkwy	To	Heritage Landing CDD
Saint Augustine, FL 32092	Billing Address	c/o Rizzetta and Company Inc 3434
Colwell Ave Ste 200 Tampa, FL 33614

Project Name	Heritage Landing: Steamboat Well Install a 20HP 230V 3PH VFD with Transducer and Rain Shield Project Description	Install a 20HP 230v 3PH VFD With Ghost Leg Power Transducer and Rainshied
Scope of Work

All VFD work is 18-25 weeks out from the time of approval. 2nd proposal to follow for electrician to wire SINE Filter and VFD

QTY	UoM/Size	Material/Description	Unit Price	Total

1.00	LUMP SUM

Heritage Landing: Install a 20HP 208V 3PH VFD with Transducer and Rain Shield

$23,965.41	$23,965.41

For internal use only			
SO#	8003017		
JOB#	460802023			
Service Line	150	Total Price	$23,965.41	
THIS IS NOT AN INVOICE
This proposal is valid for thirty (30) days unless otherwise approved by Contractor's Senior Vice President
5811 County Rd 305, Elkton, FL 32033 ph. fax

TERMS & CONDITIONS

I. The Contractor shall recognize and perform in accordance with written terms, written specifications and drawings only contained or referred to herein. All materials shall conform to bid specifications.

Work Force: Contractor shall designate a qualified representative with experience in landscape rraintenance/construction upgrades or when applicable in tree management. The vYOrkforce shall be competent and qualified, and shall be legally authorized to work in the U.S.

License and Permits: Contractor shall maintain a Landscape Contractor's license, if required by State or local law, and will con-ply with all other license requirements of the City, State and Federal Governments, as we 11 as all other requirements of law. Unless otherwise agreed upon by the parties or prohibited by law, Custorrer shall be required to obtain all necessary and required permits to allow the conmencement of the Services on the property.

Taxes: Contractor agrees to pay all applicable taxes, including sales or General Excise Tax (GET], where applicable.

	Insurance: Contractor agrees to provide General Liability Insu ranee, Automotive Liability Insurance, Worker's Corrpensation Insurance, and any other insurance required by law or Custorrer, as specffied in writing prior to commencerrent of work. If not specified, Contractor will furnish insurance with $1,000.(IDlimit of liability.

Liability: Contractor shall not be liable for any damage that occurs from Acts of God defined as extreme weather conditions, fire, earthquake, etc. and rules, regulations or restrictions irrposed by arry governrrent or governmental agency, national or regional emergency, epidemic, pandemic, health related outbreak or other medical events not caused by one or other delays or failure of perforrrance beyond the conmercially reasonable control of either party. Under these circurrstances, Cortractor shall have the right to renegotiate the terms and prices of this Contract within sixty (60) days.

	Any illegal trespass, claims and/or damages resulting from work requested that is not on property owned by Customer or not under Customer rranagement and control shall be the sole responsibility of the Customer.
s. Subcontractors: Contractor reserves the right to hire qualified subcontractors to perform specialized functions or work requiring specialized equipment.

	Additional Services: Any additional work not shown in the above specifications involving extra costs will be executed only upon signed written orders, and will become an extra charge over and above the estimate.

	Cancellation: Notice of Cancellation of work rrust be received in writing before the crew is dispatched to their location or Customer will be liable for a minimum travel charge of 5150.00 and billed to Customer.

The following sections shall apply where Contractor provides Customer with tree care services:

Tree & Sturr() Rem:>val: Trees removed will be cut as close to the ground as possible based on conditions to or next to the bottom of the tree trunk. Additional charges will be levied for unseen hazards such as, but not linited to concrete brick filled trunks, metal rods, etc. If requested mechanical grinding of visible tree stump will be done to a defined width and depth below ground level at an additional charge to the Customer. Defined backfill and landscape material may be specified. Customer shall be responsible for contacting the appropriate underground utility locator company to locate and mark underground utility lines prior to start of work Contractor is not responsible damage done to underground utilities su::h as but not limited to, cables, wires, pipes, and irrigation parts. Contractor will repair damaged irrigation lines at the Customer's expense.

Waiver of Liability: Requests for crown thinning in excess of twenty-five percent (25%) or work not in accordarce with ISA (international Society of Arboricultural) standards will require a signed waiver of liability.

Acceptance of this Contract
By executing this documenl Customer agrees to the formation of a binding contract and to the terms and conditions set forth herein. Customer represents that Contractor is authorized to perform the ¼'Ork stated on the face of this Contract. If payment has not been received by Contractor per payment terms hereunder, Contractor shall be entitled to all costs of collection, including reasonable attorneys' fees and it shall be relieved of any obligation to continue performance under this or arry other Cortract with Custorrer. Interest at a per annum rate of
1.5% per month (18% per year), or the highest rate permitted D/ law, may be charged on unpaid balance 15 days after billing.

NOTICE: FAILURE TO MAKE PAYMENT WHEN DUE FOR COMPLETED WORK ON CONSTRUCTION JOBS, MAY RESULT IN A MECHANIC'S LIEN ON THE TITLE TO YOUR PROPERTY

Customer

	Access to ..k>bsite: Customer shall provide all utilities to perform the work Customer shall furnish access to all parts of jobsite where Contractor is to perform work as required by the Contract or other functions re 1 ate d thereto, during normal business hours and other reasonable periods of time. Contractor will perform the work as reasonably practical after the Customer makes the site available for performance of the work.

Payment Terms: Upon signing this Agreement, Customer shall pay Contractor 50% of the Proposed Price and the remaining balance shall be paid by Customer to Contractor upon completion of the project unless otherwise, agreed to in writing.

Signature

Lourens Erasmus
Printed Name

Title

Date

Property Manager

December 20, 2022

Termination: This Work Order rray be terrrinated by the either party with or without cause, upon seven (7) workdays advance written notice. Customer will be required to pay for all rraterials purchased and work corr()lete to the date of termination and reasonable charges

BrightView Landscape Services, Inc. "Contractor"
Irrigation Tech-Level II

incurred in dem:>bilizing.

	Assignment: The Customer and the Contractor respectively, bind themselves, their partners, successors, assignees and legal represertatlve to the other party with respect to all covenants of this Agreement. Neither the Custorrer nor the Contractor shall assign

Signature

Juwan Lamar Dupree

Title

December 20, 2022

or transfer any interest in this Agreerrent without the written consent of the other provided, however, that consent shall not be required to assign this Agreement to any corrpany which controls, is controlled by, or is under comnon control with Contractor or in connection with assignment to an affiliate or pursuant to a merger, sale of all or substartially all of its assets or equity securities, consolidation, change of control or corporate reorganization.

Disclaimer: This proposal was estimated and priced based UJX>n a site visit and visual inspection from ground level using ordinary means, at or about the time this proposal was prepared The price quoted in this proposal f o r the work described, is the result of that ground level visual inspection and therefore our corrpany will not be liable for any additional costs or damages for additional ¼'Ork not described herein, or liable for any incidents/accidents resulting from conditions, that were not ascertainable by said ground
level visual inspection bf ordinary means at the time said inspection was performed.
Contractor cannot be held responsible for unknown or otherwise hidden defects. Any corrective work proposed herein cannot guarantee exact results. Professional engineering, architectural, and/or landscape design services ("Design Services') are not ircluded in this Agreement and shall not be provided by the Contractor. Any design defects in the Contract Documents are the sole responsibility of the Customer. If the Customer must engage a licensed engineer, architect and/or landscape design professional, any costs concerning these Design Services are to be paid by the Customer direct to the designer involved.

Printed Name	Date

Job#:	460802023		
SO#:	8003017	Proposed Price: $23,965.41	

Tab 5

HERITAGE LANDING CDD	
PROPOSAL WORKSHEET	
JOB	QTY	VENDOR	QUOTE	NOTES	ACTION	
Light 1
Lantern style with two light fixtures on one 20' pole. The lights will be more of an ambient light given off like our FPL street lights.		

Smith Electrical	

$3,793			
Light 2

Down light like our pool lights or the large black posts we have upfront at the entrance. This will be a down casting strong light field to light up the street and crosswalk area.		

Smith Electrical	

$5,389			

Smith Electrical Inc.	Estimate

Estimate #	Date	
PedCrossLt	8/24/2023	

PO Box 9023
St Augustine, FL 32085

Name / Address	
Heritage Landing CDD C/O Rizzetta & Company
3434 Colwell Ave, Suite 200
Tampa, FL 33614 cddinvoice@rizzetta.com	

Item	Description	Qty	Rate	Total	

Quote

Quote	Pedestrian Crossing Light
Supply and install materials to add (1) 20' black fiberglass pole, (2) black lantern style fixtures with (1) bull horn.

Supply and install PVC conduit, wiring and photocell.	
1

1	
3,792.52

3,087.17	
3,792.52

3,087.17	
All material is guaranteed to be as specified. All work to be completed in a substantial workmanlike manner according to specifications submitted, per standard practices.
Any variation or deviation from above specifications involving extra costs will be	Total	
$6,879.69	
executed only upon written orders, and will become an extra charge over and above
the estimate. All agreements are contingent upon strikes, accidents or delays beyond	Signature our control. Owners to carry fire, tornado and other necessary insurance.

Phone #	Fax #	E-mail	Web Site	
9048290899	904-829-0259	smithelectric08@gmail.com	staugustineelectric.com	

Project:

Location:

Cat.No:

Type:

Lamps:	Qty:

Notes:

31;1 1
("OOort -----...i

Ordering Guide Example: PTH2520 P3 A

Product Code	PTH2520	Twin	
Post diameter	P3	3" Post Mount
P4	4" Post Mount	
Finish	Black
White
Verde
Bronze
J	Green	

Specifications	
HOUSING:
356 HM high-strength, low-copper, proprietary cast aluminum alloy.
FINISH:
Thermoset polyester powdercoat is electrostatically applied after a five-stage conversion cleaning process and bonded by heat fusion thermosetting. Laboratory tested for superior weatherability and fade resistance in accordance with ASTM B117 specifications. For larger projects where a custom color is required, contact the factory for more information.
MOUNTING:
Cast Aluminum Hub mounts to a 3" OD x 3" long (P3) [if applicable) or 4" OD x 6 1/2" long (P4) [if applicable) tenon and is secured with at least (3) 5/16"-18 stainless steel set screws.
WARRANTY:
Three-year limited warranty.
Height:
17" (43cm)
Length:
39 1/4" (100 cm)
EPA:
2.05 sq. ft.

4	3	2
SMB POLE TOP MOUNTING BRACKET
CATALOG #	BRACKET DESCRIPTION
SMB-2	2 FLOOD LIGHT BRACKET

1

SOME GEOGRAPHICAL AREAS HAVE SPECIAL WIND CONDITIONS THAT CAN CREATE WIND INDUCED VIBRATIONS CAUSING A FATIGUE PROBLEM. NO METHOD HAS YET BEEN FOUND FOR PREDICTING DESTRUCTIVE LIGHTING POLE VIBRATION. THESE CONDITIONS ARE UNIQUE AND CANNOT BE GUARANTEED AGAINST, AND ARE THE RESPONSIBILITY OF A LOCAL SITE ENGINEER.
TITLE:

SHEET 1 OF 1

EPA (SQ. FT.) 1.1

34.00

SIZE:  C

D	D
30.00

A

DWG NO: SMB-2

4.00 SQ. X 11 GA TUBE

C
12.50

CATALOG:

4.00

REMOVABLE END CAP	C

4.50
3.50 SQ. X 11 GA. TUBE

(4) 3/8-16 UNC SET SCREWS AT 90°

.44 ~ THRU
FOR 3/8-16 UNC THRU BOLT (FIELD DRILLED)

A
B	B
2.38

2/19/2015

DATE:

SCALE: NONE

4.00

DRAWN: M. HARVALA
CHECKED REVISION: APPROVED: QUOTE: S.O.#
REF:

A

2 1/2 IN SCHED 40 PIPE (Ø2.88 O.D. X Ø2.47 I.D)

1.50

SECTION A-A

NOTE: SERIES SMB POLE TOP FLOOD LIGHT MOUNTING BRACKETS SLIP FIT (Ø2.38 OD) POLE TOP TENONS. EACH BRACKET HAS A MAXIMUM CAPACITY OF 1000 WATT FLOOD LIGHTS. SLIP FITTERS FOR Ø3.00 & Ø4.00 TENONS ARE AVAILABLE UPON REQUEST. SMB BRACKETS ARE FINISHED TO MATCH POLE.

SMB BRACKETS CATALOGED ARE CONSTRUCTED OF STEEL AND ARE DESIGNED FOR USE WITH STEEL OR ALUMINUM POLES. IF ALUMINUM BRACKETS ARE REQUIRED FOR ALUMINUM POLES, CONTACT YOUR REPRESENTATIVE.

270°

180°

0° HANDHOLE

A

90°

4	3	2	1

DESCRIPTION
The Lexington outdoor luminaire displays the old-fashioned charm of traditional lantern-type post top lighting, enhancing any setting with distinctive styling. As a decorative luminaire, the Lexington tastefully complements the architectural and environmental design of parks and roadways.

Streetworks

SPECIFICATION FEATURES
Construction
TOP: Hinged die-cast aluminum top with cupola cover. SCREWS: Captive retaining screw. HOUSING: Die-cast aluminum base housing. Standard color is black. Other finish colors available. Consult your Streetworks representative. 1" ANSI wattage/source label.

Optics
REFRACTOR: Injection molded acrylic retractor panels.

Electrical
SOCKET: Vertical: Base up standard on Type II, Ill and V. Horizontal: Available with Type II and Ill

horizontal reflector. Mogul-base procelain socket is field adjustable on horizontal only. 50-150W Pulse Start Metal Halide is medium-base socket standard. STARTER: Plug-in starter. TERMINAL BLOCK:Terminal block standard.

Mounting
Self-aligning pole-top fitter fits
2-3/8" and 3" O.D. tenons. Square headed 1-1/4" polymer coated mounting bolts.

Finish
Cast components finished in a Super durable black TGIC polyester powder coat paint, 2.5 mil nominal

thickness for superior protection against fade and wear. Optional colors include: bronze, grey and white. RAL and custom color matches available.

Efficiency Standards Notice Select luminaires are manufactured to USA and California efficiency regulations.

LXF/LXT
LEXINGTON

DIMENSIONS

LXF	LXT

27-1/2" [699mm]

15" [381mm]

25" [635mm]

50-150W
Pulse Start Metal Halide
50-150W
High Pressure Sodium

DECORATIVE POST TOP
LUMINAIRE

EPA
Effective Projected Area: (Sq. Ft.) 1.7

SHIPPING DATA
Approximate Net Wt:
25 lbs. (11 kgs.)

TD516008EN April 25, 2022 3:40 PM

page2	LXF/LXT LEXINGTON

PHOTOMETRIC$

150-Watt HPS
16,000-Lumen Lamp Type Ill Semi Cutoff

4

								
	/	/	
/			"			
									
	vi /	
/	.,,,--	r-----...	'\
'\.	\ \		
			( /		"\ \
A B	6	
			\ '-	./	)	)	}	
	I\ \	'\.
'\	'--	/
l	'	/ VJ			
	'\	'		/	/	V		

								

3

2
I

0

2

3

4
4	3	2	0	2	3	4

100-Watt HPS
9,500-Lumen Lamp TypeV

Footcandle Table	 Select mounting height and read across for footcandle values of each isofootcandle line. Distance in units of
 mounting height.	
Mounting	Footcandle Values for
Height	lsofootcandle Lines	
	A	B	C	D	E	

150-Watt HPS (Type 111)
10'	2.88	1.44	0.72	0.36	0.28
 12'	2.00	1.00	0.50	0.25	0.10
14'	1.50	0.75	0.37	0.18	O.D7

100-Watt HPS (Type V)
10'	1.44	0.72	0.36	0.28
 12'	1.00	0.50	0.25	0.10
14'	.75	0.37	0.18	0.07	

,P View Lexington IES files

ORDERING INFORMATION

Sample Number: LXF70SR2554
Product Family	Lamp Wattage	Lamp Type'	Ballast Type2·'	Voltage'	Distribution	
LXF=Lexington	Pulse Start Metal Halide '	P=Pulse Start Metal Halide	H=Reac./HPF	2=120V
0=208V
4=240V
7=277V
8=480V 5
9=347V
W=Multi-Tap wired 120V P=240V w/PCR wired 120V V=Multi-Tap wired 240V N=Multi-Tap wired 277V	Vertical Lamp	
LXT=Lexington w/Traditional Top	70=70W	S=High Pressure Sodium	N=Hi. Reac./NPF		22=Type II	
	10=100W		P=Hi. Reac./HPF•		33=Type 1118	
	15=150W		R=Reac./NPF		55=Type V	
	High Pressure Sodium		W=CWA		Horizontal Lamp	
	50=50W				2H=Type II	
	70=70W				3H=Type 1118	
	10=100W				4H=Type IV	
	15=150W					
Options (Add as Suffix)	
1=Single Fuse (120, 277 or 347V)
2=Double Fuse (208, 240 or 480V) 4=NEMA Photocontrol Receptacle P=Polycarbonate Lens Panels N=NEMA Ballast Bracket
S=Snap Latches for Tool-less Lamp Replacement J=Factory Installed Ladder Rest
U=UL / CSA Listed AP=Grey BK=Black BZ=Bronze WH=White
B=House Side Shield	
NOTES:
Medium-base pulse start metal halide is standard in 150W and below.
Consult a Cooper Lighting Solutions representative for lamp/ballast type/voltage compatibility.
Consult an Cooper Lighting Solutions representative for availability of EISA compliant linear reactor pulse start metal halide ballasts
Pulse start metal halide EISA compliant high reactance ballasts are available in 70, 100 and 150 watts.
Pulse start metal halide 150W 480V requires high reactance to meet EISA requirements.
Requires use of coated lamp to achieve Type Ill distribution.

Cooper Lighting Solutions 1121 Highway 74 South Peachtree City, GA 30269 P: 770-486-4800
www.cooperlighting.com

Specifications and dimensions subject to change without notice.

TD516008EN April 25, 2022 3:40 PM

Composite Pole - TR34

Designed for Post Top or Area Lighting Luminaires
Tapered composite pole shaft
Direct embedded and anchor base models
Base cover provided with AB pole
Ordering Information
Sample Catalog Number Logic

Above Grade Height Cat No.		Description TR34-10		 1O feet /3.0 M TR34-11		11 feet/3.4 M TR34-12		 12 feet /3.7 M
TR34-13 13 feet /4.0 M TR34-14 14 feet /4.3 M TR34-15 15 feet /4.6 M TR34-16 16 feet /4.9 M TR34-17 17 feet /5.2 M TR34-18 18 feet /5.5 M TR34-19 19 feet/5.8 M TR34-20 20 feet /6.1 M TR34-21 21 feet /6.4 M TR34-22 22 feet /6.7 M TR34-23 23 feet /7.0 M TR34-24 24 feet /7.3 M TR34-25 25 feet /7.6 M TR34-26 26 feet /7.9 M TR34-27 27 feet /8.3 M TR34-28 28 feet /8.5 M TR34-29 29 feet /8.8 M TR34-30  30 feet/9.1 M
Installation Method
Cat No.	Description
DE	Direct Embedded
AB	Anchor Base
Color
Cat No.	Description
BLK	Black
DBZ	Dark Bronze
DGR	Dark Green
SLV	Silver
WHT	White
GRY	Gret
cc	Custom Color - Please provide a min. 3" x 3"
color chip.

F	G

	B	C	D	
TR34	16	DE	BLK	
TR34	20	AB	DGR	
Pole	Above Grade Height	Installation Method	Color	

TXT	23
SMS	30
Surface	Tenon	Options Finish		O.D.
Surface Finish

Cat No.	Description

TXT	Natural texture of the
	reinforcing strands	
SMS	Smooth surface finish

  Tenon O.D.	
  Cat No.	Description	
23	2 3/8" (60 mm) O.D.

30	3" (76 mm) O.D.

99	Custom Tenon O.D.

  Options	
Cat No.	Description

DTC		Top pole cap and drilling for a side mounted arm(s). Provide template or drawing for hole locations.

FLD		Top pole cap. Field drill to accept a luminaire.

RC	Receptacle housing and a
NEC-approved cover with 15A GFCI receptacle. Standard location is 12"/305 mm below the top of the pole.

Other accessories are shown on the Accessories specification sheet.

ABOVE GRADE HEIGHT
20'MODEL SHOWN

© 2020 Valmont Industries, Inc. I whatley.com I +1 877.959.76781+1 803.276.5507

TR34 Tapered composite pole shaft

Direct Embedded - DE		Anchor Base Installation - AB

Shaft Length

A

18 in

460mrr

J_

Embedded
Depth

18in 460mm
--..--.---.--.--.--.-:;--

24in
/610mm

/

/

'1

embedded,

/

1/
/	/	/

10 to13 ft  3 ft /.91 M 14 to 24 ft  4 ft /1_2 M 25 to 30 ft   5 ft /1_5 M
* Embedded depths may vary per local codes, site soil conditions, drainage and very high wind conditions_
Hand hole is:
2.5"/62 mm x 5"/125 mm.

Anchor Base Dimensions for TR34

Hand hole is 2.5"/62 mm x 5"/125 mm
	Mounting slots are .75"/19 mm x_15"/38 mm for 8" bolt circle and 1"/25 mm x 1_5"/38 mm for 10" and 12" bolt circle
Conduit entry hole in base plate is 4_0"/100 mm

Specifications
POLE SHAFT
The pole shaft shall be round tapered, smooth with _a 14"/3_5 mm per foot taper_The hand hole shall be 2_5"/62 mm x 5"/125 mm with a cover_The shaft shall be constructed of continuous fiberglass filament combined with a thermosetting resin_ The glass filament shall be helically wound at alternating high and low angle layers for maximum compressive and bending strength_The hand hole area and hardware attachment areas shall be reinforced_
The butt end of the embedded-type post shall be enlarged and oval to increase the resistance to rotation and provide maximum ground bearing resistance (anti-lift)_The post shall be non-conductive and chemically inert_
PERFORMANCE CRITERIA
The post shall be designed with a minimum safety factor of_15:1and have no more than a 15% deflection at full wind loading_The post shall deflect no more than 2_5% of the above-ground length with 100 lbs of lateral top load_Poles shall be tested and rated per
ANSI C136_20-2012_
DIRECT EMBEDDED INSTALLATION
Direct embedded poles shall have a 2_5 inch (62 mm) by 6 inch
(152 mm) slot for conduit entrance 24 inches (610 mm) below finished grade_Embedded depths may vary per local codes.site soil conditions, drainage and very high wind conditions_
ANCHOR BASE
Anchor bases shall be constructed of primed and painted aluminum or galvanized steel. The base shall be factory bonded to the pole_
TENON
A painted galvanized steel or aluminum tenon shall be firmly bonded to the pole for mounting a post-top luminaire or arm_
FINISH
The surface of the post shall be uniform and consistent for the entire length of the post. A UV-resistant catalyzed urethane coating shall be extremely durable and retains its gloss after a 5000 hour exposure test per ASTM G154, with no dulling or chalking of the surface_
BASE COVER
For anchor-base poles, the standard base cover shall be a round or square two-piece molded ABS cover_This base cover shall be corrosion free and painted to match the pole_Base covers are not included with direct-embedded poles_

Shaft Length	Bolt Circle (A)	Base Plate Size (B)	Anchor Bolts	
10' - 13'	8"/203 mm	7_5"/190 mm	5/8" x 21"	
14' - 26'	10"/254 mm	10"/254 mm	3/4" x 30"
27' - 30'	12"/304 mm	1_15"/292 mm	3/4" x 30"
Wind Loading Data

WIND SPEED (MPH) WITH 3 SECOND GUST FACTOR

Cat	No_ Description	WT	90	100	110	120	130	140	150	
10	10 feet/3_10 M	26	11.8	9.2	7.5	6.2	5_2	4.4	3_8	
11	11 feet/3_35 M	29	11.3	8.8	7.2	5.9	5_0	4.2	3_6	
12	12 feet/3_66 M	31	10.2	8.0	6.5	5.3	4.4	3.7	3_2	
13	13 feet/3_96 M	34	9.4	7.4	5.9	4.9	4_1	3.4	2_9	
14	14 feet/4.27 M	37	8.7	6.8	5.5	4.5	3_7	3.1	2_6	
15	15 feet/4_57 M	38	9.2	8.0	6.5	5.3	4.4	3.7	3_1	
16	16 feet/4_88 M	42	9_3	7.3	5.9	4.8	4_0	3.3	2_8	
17	17 feet/5.18 M	45	8.6	6.7	5.4	4.4	3_6	3.0	2_5	
18	18 feet/5.49 M	49	7.9	6.1	4.9	3.9	3_2	2.7	2_2	
19	19 feet/5.79 M	51	7.2	5.6	4.4	3.6	2_9	2.4	2_0	
20	20 feet/6.10 M	52	6_6	5.1	4.0	3.2	2_6	2.1 _18	
21	21 feet/6.40 M	75	8_2	6.4	5.1	4.1	3_4	2.8  2_3	
22 22 feet/6_71 M	77	7.5	5.8	4.6	3.7	3_0	2.5 2_1	
23 23 feet/7.01 M	80	6_9 5.3	4.2	3.3	2_7	2.2 _18	
24 24 feet/7.32 M	83	6_3 4.9	3.8	3.0	2_4	2.0 _16	
25 25 feet/7.62 M	85	5_8 4.4	3.4	2.7	2_1	1.7 _13	
26 26 feet/7.92 M	88	5_3 4.0	3.1	2.4 _19	1.5 _1 1	
27 27 feet/8_32 M	91	4_9 3.6	2.8	2.1 _1 7	1.3 0_9	
28 28 feet/8_53 M	93	4.4 3.3	2.5	1.9  1.4	1.1	o_7	
29 29 feet/8_84 M	96	3_9 2.9	2.1	1.6 _12	0.9	0_5	
30 30 feet/9.14 M	99	3_5 2.5	1.8	1.3 _10	0.7	0_3	
Wind speed values are for a 3 second gust per ASCE. Calculated per ANSI C136_20-2012_Assumes load 12 inches above the pole top_ Safety factor =_15:_1 Maximum weight for tenon mount is 100 lbs_ Contact factory for AASHTO or specific local codes_
valmont
STRUCTURES

© 2020 Valmont Industries, Inc_ All rights reserved_Whatley has a policy of continuous product improvement and development. As a result, certain changes in standard equipment, options, price, etc_ may have occurred after the publication of this document. Some photographs and specifications may not be identical to current production_Whatley reserves the right to change product design and specifications at any time without incurring obligations_
whatley.com I +1 877_959_76781+1 803_276_5507 SPC7394_0420

Smith Electrical Inc.	Estimate

Estimate #	Date	
Heritage	12/1/2023	

PO Box 9023
St Augustine, FL 32085

Name / Address	
Heritage Landing CDD C/O Rizzetta & Company
3434 Colwell Ave, Suite 200
Tampa, FL 33614 cddinvoice@rizzetta.com	

Item	Description	Qty	Rate	Total	
Quote	Supply and install 20' black fiberglass pole with bullhorn and (2) 100w LED fixtures.		5,388.77	5,388.77	
All material is guaranteed to be as specified. All work to be completed in a substantial workmanlike manner according to specifications submitted, per standard practices.
Any variation or deviation from above specifications involving extra costs will be	Total	
$5,388.77	
executed only upon written orders, and will become an extra charge over and above
the estimate. All agreements are contingent upon strikes, accidents or delays beyond	Signature our control. Owners to carry fire, tornado and other necessary insurance.

Phone #	Fax #	E-mail	Web Site	
9048290899	904-829-0259	smithelectric08@gmail.com	staugustineelectric.com	

Project		
Catalog #		
Type		

Prepared by		
Notes		
Date		

Lumark
Navion
Area / Site Luminaire

Product Features

LumenSafe Technology  Light ARchitectTM

Interactive Menu
Ordering Information page 2
Mounting Details page 3
Optical Configurations page 3
Product Specifications page 4
Energy and Performance Data page 4
Control Options page 7

Product Certifications

1	1

 BAA 

BUY AMERICAN ACT

L

2

Quick Facts
Patented, high-efficiency AccuLED Optics system provides uniform illumination in 16 different optical distributions
Lumen packages range from 4,700 - 50,000 nominal lumens (30W - 380W)
Tool-less entry; hinged removable power door for easy maintenance
Efficacies up to 158 lumens per watt
Dimensional Details

Filler Plate

1, 2 or 3 Light Squares	5 Light Squares

5-7/32" [132mm]

8-7/8" [225mm]

4, 5 or 6 Light Squares

Connected Systems
WaveLinx
Enlighted

Light Square

21-1/2" [546mm]

or 4 Light Squares

5-7/32" [132mm]

15" [381mm]

27-5/8" [701mm]

3, 5 or 6 Light Squares

33-5/8" [854mm]

additional product diagrams

NOTES:
Visit https://www.designlights.org/search/ to confirm qualification. Not all product variations are DLC qualified.
IDA Certified for 3000K CCT and warmer only.

Ordering Information
SAMPLE ORDER NUMBER: NAV-SA1C-740-U-T3-AP

Product Family 1, 2	Light Engine	Color Temperature	Voltage	Distribution	Mounting	Finish	
NAV=Navion
BAA-NAV=Navion Buy American Act Compliant 23
TAA-NAV=Navion Trade Agreements Act Compliant 23	Configuration	Drive Current	722=70CRI, 2200K
727=70CRI, 2700K
730=70CRI, 3000K
735=70CRI, 3500K
740=70CRI, 4000K
750=70CRI, 5000K
760=70CRI, 6000K
827=80CRI, 2700K
830=80CRI, 3000K
835=80CRI, 3500K
AMB=590nm Amber 3	U=Universal (120-277V)
9=347V 4
8=480V 5
DV=277-480V DuraVolt Drivers 5, 25, 26	T2=Type II
T2R=Type II Roadway
T3=Type III
T3R=Type III Roadway T4FT=Type IV Forward Throw T4W=Type IV Wide 5NQ=Type V Narrow 5MQ=Type V Square Medium 5WQ=Type V Square Wide SL2=Type II w/Spill Control SL3=Type III w/Spill Control SL4=Type IV w/Spill Control
SLL=90° Spill Light Eliminator Left SLR=90° Spill Light Eliminator Right RW=Rectangular Wide Type I AFL=Automotive Front Line	[Blank]=Standard Mast Arm Slipfitter
AI=22" Upsweep Mast Arm 6 A15=15" Straight Mast Arm 6 ALJS15=Adjustable Slipfitter (Factory set at 15° tilt) ALJS25=Adjustable Slipfitter (Factory set at 25° tilt) ALJS45=Adjustable Slipfitter (Factory set at 45° tilt)	AP=Grey BZ=Bronze BK=Black DP=Dark Platinum GM=Graphite
Metallic
WH=White	
	SA1=1 Square SA2=2 Squares SA3=3 Squares SA4=4 Squares SA5=5 Squares SA6=6 Squares	A=615mA B=800mA C=1050mA (1A) D=1200mA (1.2A)						
Options (Add as Suffix)	
10MSP=10kV MOV Surge Protective Device	AHD145=After Hours Dim, 5 Hours 11
10K=10kV UL 1449 Fused Surge Protective Device	AHD245=After Hours Dim, 6 Hours 11
20MSP=20kV MOV Surge Protective Device	AHD255=After Hours Dim, 7 Hours 11
20K=20kV UL 1449 Surge Protective Device	AHD355=After Hours Dim, 8 Hours 11
2L=Two Circuits 7	SPB1=Dimming Occupancy Sensor with Bluetooth Interface, <8’ Mounting 22
L90=Optics Rotated 90° Left	SPB2=Dimming Occupancy Sensor with Bluetooth Interface, 8’-20’ Mounting 22
R90=Optics Rotated 90° Right	SPB4=Dimming Occupancy Sensor with Bluetooth Interface, 21’-40’ Mounting 22
HSS=House Side Shield 8	MS-L08=Motion Sensor for ON/OFF Operation, Up to 8' Mounting Height 12, 13
HA=50°C High Ambient Temperature 9	MS-L20=Motion Sensor for ON/OFF Operation, 9' - 20' Mounting Height 12, 13
IP66=IP66 Rated	MS-L40=Motion Sensor for ON/OFF Operation, 21' - 40' Mounting Height 12, 13
K=Level Indicator	MS/X-L08=Motion Sensor for Bi-Level Operation, Up to 8' Mounting Height 12, 13, 14 LCF=Light Square Trim Plate Painted to Match Housing	MS/X-L20=Motion Sensor for Bi-Level Operation, 9' - 20' Mounting Height 12, 13, 14 CC=Coastal Construction finish 21	MS/X-L40=Motion Sensor for Bi-Level Operation, 21' - 40' Mounting Height 12, 13, 14
CE=CE Marking 9, 10	MS/DIM-L08=Motion Sensor for Dimming Operation, Up to 8' Mounting Height 12, 13
PR=NEMA 3-PIN Twistlock Photocontrol Receptacle	MS/DIM-L20=Motion Sensor for Dimming Operation, 9' - 20' Mounting Height 12, 13
PR7=NEMA 7-PIN Twistlock Photocontrol Receptacle	MS/DIM-L40=Motion Sensor for Dimming Operation, 21' - 40' Mounting Height 12, 13
FADC=Field Adjustable Dimming Controller 27	LWR-LW=Enlighted Wireless Sensor, 8' - 16' Mounting Height 12, 15
LWR-LN=Enlighted Wireless Sensor, 16' - 40' Mounting Height 12, 15
[See Table Below]=LumenSafe Integrated Network Security Camera 16	
Accessories (Order Separately) 24	
OA/RA1013=Twistlock Receptacle Shorting Cap	MA1018-XX=2@180° Tenon Adapter for 2-3/8" O.D. Tenon
OA/RA1014=NEMA Twistlock Photocontrol - 120V	A15-XX=15" Straight Mast Arm Kit 6
OA/RA1016=NEMA Twistlock Photocontrol - Multi-Tap	ALJS15-XX=Adjustable Slipfitter Kit (Factory set at 15° tilt)
OA/RA1027=NEMA Twistlock Photocontrol - 480V	ALJS25-XX=Adjustable Slipfitter Kit (Factory set at 25° tilt)
OA/RA1201=NEMA Twistlock Photocontrol - 347V	ALJS45-XX=Adjustable Slipfitter Kit (Factory set at 45° tilt)
MA1010-XX=Single Tenon Adapter for 3-1/2" O.D. Tenon	LS/HSS=House Side Shield 8, 18
MA1011-XX=2@180° Tenon Adapter for 3-1/2" O.D. Tenon	FSIR-100=Wireless Configuration Tool for Motion Sensor 19
MA1017-XX=Single Tenon Adapter for 2-3/8" O.D. Tenon	WOLC-7P-10A=WaveLinx Outdoor Control Module (7-PIN) 20	
NOTES:
DesignLights Consortium® Qualified. Refer to www.designlights.org Qualified Products List under Family Models for details.
Customer is responsible for engineering analysis to confirm pole and fixture compatibility for applications. Refer to installation instructions and pole white paper WP513001EN for additional support information.
Only available at Drive Current (A) which will be supplied at 500mA.
Not available with sensor options at 1.2A drive current. Not available in combination with HA high ambient and sensor options at 1A drive current.
480V not to be used with ungrounded or impedance grounded systems.
Round pole adapter and mounting hardware included. Type M drill pattern.
Option available only with 4 and 6 Square configurations. Low-level output varies. Consult factory. Option not available in combination with high voltage (9 or 8) and sensor options (PR, PR7, AHD, MS, LWR, LumenSafe). No terminal block with 2L option.
House side shield not for use on 5NQ, 5MQ, 5WQ, or RW distributions. The Light Square Trim Plate is painted black when HSS option is selected.
Not available with 1.2A drive current or Amber color temperature (AMB).
Only available at Universal (U) voltage. Not available with sensor or controls options (PR, PR7, AHD, MS, LWR, LumenSafe).
Requires the use of Photocontrol Receptacle (PR or PR7) and a photocontrol accessory. See After Hours Dim Supplemental Guide for additional information.
Controls system is not available with photocontrol receptacle (PR or PR7) or other controls systems (MS or LWR).
Utilizes the Wattstopper sensor FSP-211.
Available with 4, 5, or 6 square configurations. Replace "X" with number of squares in low output modes. Maximum two squares in low output mode.
Enlighted wireless sensors are factory installed and require network components LWP-EM-1, LWP-GW-1, and LWP-PoE8 in appropriate quantities. See website for Enlighted application information.
All configurations require 15-in wide housing size. If 1-3 light square is selected, filler plates will be used. LumenSafe not available at high voltage (9 or 8) or High Ambient (HA). When ordered with Type V optic, a factory-installed light shield will be provided.
Replace XX with paint color.
Must order one per light square when ordering as a field-installable accessory.
This tool enables adjustment to Motion Sensor (MS) parameters including high and low modes, sensitivity, time delay, cutoff and more. Consult your lighting representative for more information.
Requires 7-PIN NEMA twistlock photocontrol receptacle (PR7) option. The WOLC-7 cannot be used in conjunction with other controls systems (MS or LWR). Only for use at 120-347V voltages.
Coastal construction finish salt spray tested to over 5,000-hours per ASTM B117, with a scribe rating of 9 per ASTM D1654.
Smart device with mobile application required to change system defaults. See controls section for details.
Only product configurations with these designated prefixes are built to be compliant with the Buy American Act of 1933 (BAA) or Trade Agreements Act of 1979 (TAA), respectively. Please refer to DOMESTIC PREFERENCES website for more information. Components shipped separately may be separately analyzed under domestic preference requirements.
Accessories sold separately will be separately analyzed under domestic preference requirements. Consult factory for further information.
DuraVolt drivers feature added protection from power quality issues such as loss of neutral, transients and voltage fluctuations. Visit www.signify.com/duravolt for more information.
Not available in 1 square configuration at 800mA and below. Not available with any control option except SPB.
Cannot be used with PR7 or other motion response control options.	

LumenSafe Integrated Network Security Camera Technology Options (Add as Suffix)
Product Family	Camera Type	Data Backhaul	
L=LumenSafe Technology	D=Dome Camera, Standard H=Dome Camera, Hi-Res Z=Dome Camera, Remote PTZ	C=Cellular, Customer Installed SIM Card A=Cellular, Factory Installed AT&T SIM Card V=Cellular, Factory Installed Verizon SIM Card	S=Cellular, Factory Installed Sprint SIM Card W=Wi-Fi Networking w/ Omni-Directional Antenna E=Ethernet Networking	

LumenSafe Technology				

Mounting Details
Type "M"
2-5/16"
[59mm]

Adjustable Slipfitter Offset Arm

45°

16" [406mm]

3/4" [19mm] Dia. Hole
2-7/16" [62mm]

4-7/8" [124mm]

(2) 5/8" [16mm]
Dia. Holes

Upsweep Arm
Upsweep Arm

4º

7" [178mm]

32º

2-3/8"
Rise 8-1/8"	[60mm]
[206mm]	O.D.

10-3/4" [273mm]

21-1/2" [546mm]

15" Straight Arm	Effecitve Projected Area (EPA)

7" [178mm]

2-3/8"
[60mm]

14-13/16" [376mm]

Configuration	Fixture Only EPA
(Sq. Ft.)	Fixture and Upsweep Arm EPA
(Sq. Ft.)	
1 Square	0.8	1.2	
2 Squares	1.0	1.3	
3 Squares	1.2	1.5	
4 Squares	1.2	1.5	
5 Squares	1.4	1.7	
6 Squares	1.4	1.7	

Optical Configurations
Orientation
Standard	Optics Rotated Left @ 90˚	Optics Rotated Right @ 90˚

Street Side

House Side

Street Side

House Side

Street Side

House Side

Distributions

Asymmetric Area Distributions
T2	SL2	T3	SL3	T4FT	T4W	SL4
(Type II)	(Type II with Spill Control)	(Type III)	(Type III with Spill Control)  (Type IV Forward Throw)	(Type IV Wide)	(Type IV with Spill Control)

Asymmetric Roadway Distributions			Symmertric Distributions		
RW	T2R	T3R	5NQ	5MQ	5WQ	
(Rectangular Wide Type I)	(Type II Roadway)	(Type III Roadway)	(Type V Square Narrow)	(Type V Square Medium)	(Type V Square Wide)	

	Specialized Distributions		
AFL	SLL	SLR	
(Automotive Frontline)	(90° Spill Light Eliminator Left)	(90° Spill Light Eliminator Right)	

Product Specifications
Construction
Die-cast aluminum housing and door
Extruded aluminum heat sink
Tool-less entry, hinged removable power tray door

Optics
Light square are IP66 enclosure rated
Precision molded polycarbonate optics
IDA certified (3000K CCT and warmer only)

Electrical
-40°C minimum operating temperature
40°C maximum operating temperature

Energy and Performance Data

View Navion IES files

Drive Current	Ambient Temperature	TM-21 Lumen Maintenance (60,000 Hours)	Projected L70 (Hours)	
Up to 1A	Up to 50ºC	> 95%	416,000	
1.2A	Up to 40°C	> 90%	205,000	

Lumen Maintenance

>.9 power factor
<20% total harmonic distortion
0-10V dimming driver standard

Mounting
Four-bolt / two-bracket slipfitter with cast-in pipe stop and level steps at 2.5° increments
Fixed-in-place bird guard seals around 1-1/4" or 2" mounting arms

Finish
Housing and cast parts finished in five-stage super TGIC polyester powder coat paint, 2.5 mil nominal thickness

Heat sink is anodized aluminum

Shipping Data
1 Square 17 lbs. (7.7kgs.)
2 Squares 22 lbs. (10.0 kgs.)
3 Squares 26 lbs. (11.8 kgs.)
4 Squares 31 lbs (14.1 kgs.)
5 Squares 34 lbs. (15.4 kgs.)
6 Squares 36 lbs. (16.3 kgs.)

Warranty
Five year limited warranty, consult website for details. www.cooperlighting.com/legal

Ambient Temperature	Lumen Multiplier	
0°C	1.02	
10°C	1.01	
25°C	1.00	
40°C	0.99	
50°C	0.97	

Lumen Multiplier

FADC Settings	FADC Settings	FADC Settings	FADC Settings	
SA1-SA3 (A, B, C, D Drive Current)	SA4A	SA4C-D	SA5-SA6 (A, B, C, D Drive Current)	

FADC Position	Percent of Typical
Lumen Output	
1	25%	
2	48%	
3	56%	
4	65%	
5	75%	
6	80%	
7	85%	
8	90%	
9	95%	
10	100%	

 	

FADC Position	Percent of Typical Lumen Output	
1	25%	
2	48%	
3	56%	
4	65%	
5	75%	
6	80%	
7	85%	
8	90%	
9	95%	
10	100%	

	

FADC Position	Percent of Typical Lumen Output	
1	14%	
2	25%	
3	32%	
4	43%	
5	49%	
6	57%	
7	65%	
8	72%	
9	80%	
10	100%	

	
FADC Position	Percent of Typical
Lumen Output	
1	14%	
2	25%	
3	32%	
4	43%	
5	49%	
6	57%	
7	65%	
8	72%	
9	80%	
10	100%	

Number of Light Squares	SA1A	SA1B	SA1C	SA1D	SA2A	SA2B	SA2C	SA2D	SA3A	SA3B	SA3C	SA3D	
Square Count	1	1	1	1	2	2	2	2	3	3	3	3	
Drive Current (mA)	615	800	1050	1200	615	800	1050	1200	615	800	1050	1200	
Power (Watts)	34	44	59	67	66	85	113	129	96	124	166	191	
Input Current @ 120V (A)	0.30	0.39	0.51	0.51	0.58	0.77	1.02	1.16	0.86	1.13	1.53	1.78	
Input Current @ 208V (A)	0.17	0.22	0.29	0.33	0.34	0.44	0.56	0.63	0.49	0.62	0.82	0.93	
Input Current @ 240V (A)	0.15	0.19	0.26	0.29	0.30	0.38	0.48	0.55	0.43	0.54	0.71	0.80	
Input Current @ 277V (A)	0.14	0.17	0.23	0.25	0.28	0.36	0.42	0.48	0.41	0.47	0.61	0.70	
Input Current @ 347V (A)	0.11	0.15	0.17	0.20	0.19	0.24	0.32	0.39	0.30	0.38	0.50	0.57	
Input Current @ 480V (A)	0.08	0.11	0.14	0.15	0.15	0.18	0.24	0.30	0.24	0.29	0.37	0.43	
Distribution 1	

T2	Lumens	4,681	5,741	7,106	7,796	9,334	11,447	14,167	15,541	13,881	17,022	21,069	23,111	
	BUG Rating	B1-U0-G1	B1-U0-G2	B1-U0-G2	B1-U0-G2	B2-U0-G2	B2-U0-G2	B2-U0-G3	B2-U0-G3	B2-U0-G3	B2-U0-G3	B3-U0-G3	B3-U0-G4	
	Lumens per Watt	138	130	120	116	141	135	125	120	145	137	127	121	

T2R	Lumens	5,012	6,146	7,607	8,345	9,993	12,255	15,168	16,639	14,862	18,225	22,556	24,744	
	BUG Rating	B1-U0-G1	B1-U0-G1	B1-U0-G2	B1-U0-G2	B1-U0-G2	B2-U0-G2	B2-U0-G2	B2-U0-G2	B2-U0-G2	B2-U0-G2	B3-U0-G3	B3-U0-G3	
	Lumens per Watt	147	140	129	125	151	144	134	129	155	147	136	130	

T3	Lumens	4,784	5,866	7,261	7,966	9,539	11,697	14,480	15,883	14,186	17,395	21,531	23,619	
	BUG Rating	B1-U0-G1	B1-U0-G2	B1-U0-G2	B1-U0-G2	B2-U0-G2	B2-U0-G2	B2-U0-G2	B2-U0-G3	B2-U0-G2	B3-U0-G3	B3-U0-G3	B3-U0-G4	
	Lumens per Watt	141	133	123	119	145	138	128	123	148	140	130	124	

T3R	Lumens	4,865	5,966	7,384	8,100	9,699	11,894	14,721	16,149	14,425	17,689	21,893	24,016	
	BUG Rating	B1-U0-G1	B1-U0-G2	B1-U0-G2	B1-U0-G2	B1-U0-G2	B2-U0-G2	B2-U0-G3	B2-U0-G3	B2-U0-G3	B2-U0-G3	B3-U0-G4	B3-U0-G4	
	Lumens per Watt	143	136	125	121	147	140	130	125	150	143	132	126	

T4FT	Lumens	4,821	5,911	7,316	8,026	9,612	11,787	14,589	16,004	14,294	17,529	21,694	23,799	
	BUG Rating	B1-U0-G2	B1-U0-G2	B1-U0-G2	B1-U0-G3	B2-U0-G3	B2-U0-G3	B2-U0-G3	B2-U0-G3	B2-U0-G3	B3-U0-G4	B3-U0-G4	B3-U0-G4	
	Lumens per Watt	142	134	124	120	146	139	129	124	149	141	131	125	

T4W	Lumens	4,727	5,796	7,175	7,870	9,423	11,556	14,302	15,690	14,015	17,185	21,270	23,333	
	BUG Rating	B1-U0-G2	B1-U0-G2	B1-U0-G2	B2-U0-G2	B2-U0-G2	B2-U0-G2	B2-U0-G3	B3-U0-G3	B2-U0-G3	B3-U0-G3	B3-U0-G4	B3-U0-G4	
	Lumens per Watt	139	132	122	117	143	136	127	122	146	139	128	122	

SL2	Lumens	4,689	5,750	7,116	7,807	9,350	11,464	14,189	15,566	13,903	17,049	21,102	23,149	
	BUG Rating	B1-U0-G2	B1-U0-G2	B1-U0-G2	B2-U0-G3	B2-U0-G3	B2-U0-G3	B2-U0-G3	B3-U0-G3	B2-U0-G3	B3-U0-G4	B3-U0-G4	B3-U0-G4	
	Lumens per Watt	138	131	121	117	142	135	126	121	145	137	127	121	

SL3	Lumens	4,777	5,858	7,251	7,954	9,524	11,680	14,455	15,857	14,164	17,367	21,496	23,581	
	BUG Rating	B1-U0-G2	B1-U0-G2	B1-U0-G2	B1-U0-G2	B1-U0-G3	B2-U0-G3	B2-U0-G3	B2-U0-G3	B2-U0-G3	B2-U0-G3	B3-U0-G4	B3-U0-G4	
	Lumens per Watt	140	133	123	119	144	137	128	123	148	140	129	123	

SL4	Lumens	4,563	5,595	6,926	7,597	9,098	11,155	13,808	15,147	13,529	16,590	20,535	22,526	
	BUG Rating	B1-U0-G2	B1-U0-G2	B1-U0-G3	B1-U0-G3	B1-U0-G3	B1-U0-G3	B2-U0-G4	B2-U0-G4	B2-U0-G4	B2-U0-G4	B2-U0-G5	B2-U0-G5	
	Lumens per Watt	134	127	117	113	138	131	122	117	141	134	124	118	

5NQ	Lumens	4,917	6,029	7,462	8,186	9,803	12,022	14,879	16,323	14,579	17,877	22,126	24,274	
	BUG Rating	B2-U0-G1	B2-U0-G1	B3-U0-G1	B3-U0-G1	B3-U0-G1	B3-U0-G1	B3-U0-G2	B3-U0-G2	B3-U0-G2	B4-U0-G2	B4-U0-G2	B4-U0-G2	
	Lumens per Watt	145	137	126	122	149	141	132	127	152	144	133	127	

5MQ	Lumens	5,094	6,247	7,731	8,481	10,156	12,455	15,415	16,910	15,103	18,521	22,923	25,147	
	BUG Rating	B3-U0-G1	B3-U0-G1	B3-U0-G2	B3-U0-G2	B3-U0-G2	B4-U0-G2	B4-U0-G2	B4-U0-G2	B4-U0-G2	B4-U0-G2	B5-U0-G3	B5-U0-G3	
	Lumens per Watt	150	142	131	127	154	147	136	131	157	149	138	132	

5WQ	Lumens	4,976	6,102	7,553	8,285	9,921	12,166	15,058	16,518	14,755	18,092	22,394	24,565	
	BUG Rating	B3-U0-G1	B3-U0-G1	B3-U0-G2	B3-U0-G2	B4-U0-G2	B4-U0-G2	B4-U0-G2	B4-U0-G2	B4-U0-G2	B5-U0-G3	B5-U0-G3	B5-U0-G3	
	Lumens per Watt	146	139	128	124	150	143	133	128	154	146	135	129	

SLL/ SLR	Lumens	4,225	5,181	6,412	7,035	8,423	10,328	12,784	14,023	12,526	15,360	19,011	20,854	
	BUG Rating	B1-U0-G2	B1-U0-G2	B1-U0-G2	B1-U0-G3	B1-U0-G3	B2-U0-G3	B2-U0-G3	B2-U0-G3	B2-U0-G3	B2-U0-G4	B2-U0-G4	B3-U0-G4	
	Lumens per Watt	124	118	109	105	128	122	113	109	130	124	115	109	

RW	Lumens	4,887	5,994	7,418	8,138	9,745	11,950	14,791	16,224	14,492	17,770	21,995	24,128	
	BUG Rating	B2-U0-G1	B3-U0-G1	B3-U0-G1	B3-U0-G1	B3-U0-G1	B3-U0-G2	B4-U0-G2	B4-U0-G2	B4-U0-G2	B4-U0-G2	B4-U0-G2	B4-U0-G2	
	Lumens per Watt	144	136	126	121	148	141	131	126	151	143	132	126	

AFL	Lumens	4,901	6,009	7,438	8,159	9,771	11,981	14,829	16,268	14,532	17,818	22,054	24,193	
	BUG Rating	B1-U0-G1	B1-U0-G1	B1-U0-G1	B1-U0-G1	B1-U0-G1	B2-U0-G2	B2-U0-G2	B2-U0-G2	B2-U0-G2	B2-U0-G2	B3-U0-G2	B3-U0-G2	
	Lumens per Watt	144	137	126	122	148	141	131	126	151	144	133	127	
NOTES: 1. Photometric data published here for 740, 750, 760 Color Temperature options. For other options, refer to published IES files on product webpage or Supplemental Performance Tables.

Power and Lumens (4-6 Light Squares)

Number of Light Squares	SA4A	SA4B	SA4C	SA4D	SA5A	SA5B	SA5C	SA5D	SA6A	SA6B	SA6C	SA6D	
Square Count	4	4	4	4	5	5	5	5	6	6	6	6	
Drive Current (mA)	615	800	1050	1200	615	800	1050	1200	615	800	1050	1200	
Power (Watts)	129	171	225	258	162	210	279	320	193	249	333	382	
Input Current @ 120V (A)	1.16	1.54	2.03	2.31	1.44	1.90	2.55	2.94	1.73	2.26	3.06	3.56	
Input Current @ 208V (A)	0.65	0.88	1.11	1.27	0.84	1.06	1.37	1.57	0.99	1.24	1.64	1.87	
Input Current @ 240V (A)	0.56	0.76	0.96	1.10	0.74	0.92	1.19	1.35	0.87	1.08	1.41	1.61	
Input Current @ 277V (A)	0.52	0.72	0.83	0.96	0.69	0.83	1.03	1.18	0.81	0.95	1.23	1.39	
Input Current @ 347V (A)	0.39	0.49	0.64	0.78	0.49	0.63	0.82	0.96	0.60	0.77	1.00	1.15	
Input Current @ 480V (A)	0.30	0.37	0.48	0.60	0.38	0.48	0.61	0.73	0.48	0.59	0.75	0.85	
Distribution 1	

T2	Lumens	18,696	22,927	28,377	31,129	23,043	28,257	34,975	38,366	27,605	33,851	41,897	45,962	
	BUG Rating	B3-U0-G3	B3-U0-G4	B3-U0-G4	B3-U0-G4	B3-U0-G4	B3-U0-G4	B3-U0-G4	B3-U0-G5	B3-U0-G4	B3-U0-G4	B3-U0-G5	B3-U0-G5	
	Lumens per Watt	145	134	126	121	142	135	125	120	143	136	126	120	

T2R	Lumens	20,017	24,545	30,380	33,327	24,669	30,251	37,442	41,074	29,554	36,241	44,856	49,206	
	BUG Rating	B2-U0-G3	B3-U0-G3	B3-U0-G4	B3-U0-G4	B3-U0-G3	B3-U0-G4	B3-U0-G4	B3-U0-G4	B3-U0-G3	B3-U0-G4	B3-U0-G4	B3-U0-G5	
	Lumens per Watt	155	144	135	129	152	144	134	128	153	146	135	129	

T3	Lumens	19,106	23,430	28,999	31,811	23,548	28,877	35,741	39,207	28,210	34,593	42,816	46,969	
	BUG Rating	B3-U0-G3	B3-U0-G4	B3-U0-G4	B3-U0-G4	B3-U0-G4	B3-U0-G4	B3-U0-G5	B3-U0-G5	B3-U0-G4	B3-U0-G4	B3-U0-G5	B4-U0-G5	
	Lumens per Watt	148	137	129	123	145	138	128	123	146	139	129	123	

T3R	Lumens	19,428	23,824	29,488	32,346	23,944	29,363	36,343	39,868	28,685	35,175	43,537	47,759	
	BUG Rating	B2-U0-G3	B3-U0-G4	B3-U0-G4	B3-U0-G4	B3-U0-G4	B3-U0-G4	B3-U0-G5	B3-U0-G5	B3-U0-G4	B3-U0-G5	B3-U0-G5	B3-U0-G5	
	Lumens per Watt	151	139	131	125	148	140	130	125	149	141	131	125	

T4FT	Lumens	19,251	23,607	29,219	32,054	23,727	29,097	36,014	39,506	28,425	34,857	43,142	47,326	
	BUG Rating	B3-U0-G4	B3-U0-G4	B3-U0-G5	B3-U0-G5	B3-U0-G4	B3-U0-G5	B3-U0-G5	B3-U0-G5	B3-U0-G5	B3-U0-G5	B3-U0-G5	B4-U0-G5	
	Lumens per Watt	149	138	130	124	146	139	129	123	147	140	130	124	

T4W	Lumens	18,876	23,146	28,648	31,427	23,264	28,528	35,310	38,734	27,868	34,174	42,298	46,400	
	BUG Rating	B3-U0-G4	B3-U0-G4	B3-U0-G4	B3-U0-G5	B3-U0-G4	B3-U0-G4	B3-U0-G5	B4-U0-G5	B3-U0-G4	B3-U0-G5	B4-U0-G5	B4-U0-G5	
	Lumens per Watt	146	135	127	122	144	136	127	121	144	137	127	121	

SL2	Lumens	18,726	22,963	28,421	31,178	23,080	28,302	35,030	38,426	27,649	33,904	41,964	46,034	
	BUG Rating	B3-U0-G4	B3-U0-G4	B3-U0-G5	B3-U0-G5	B3-U0-G4	B3-U0-G5	B3-U0-G5	B4-U0-G5	B3-U0-G5	B3-U0-G5	B4-U0-G5	B4-U0-G5	
	Lumens per Watt	145	134	126	121	142	135	126	120	143	136	126	121	

SL3	Lumens	19,075	23,391	28,952	31,760	23,511	28,831	35,684	39,145	28,166	34,538	42,749	46,894	
	BUG Rating	B2-U0-G4	B3-U0-G4	B3-U0-G5	B3-U0-G5	B3-U0-G4	B3-U0-G5	B3-U0-G5	B3-U0-G5	B3-U0-G5	B3-U0-G5	B3-U0-G5	B3-U0-G5	
	Lumens per Watt	148	137	129	123	145	137	128	122	146	139	128	123	

SL4	Lumens	18,222	22,345	27,656	30,339	22,459	27,540	34,086	37,392	26,905	32,992	40,835	44,795	
	BUG Rating	B2-U0-G4	B2-U0-G5	B3-U0-G5	B3-U0-G5	B2-U0-G5	B3-U0-G5	B3-U0-G5	B3-U0-G5	B3-U0-G5	B3-U0-G5	B3-U0-G5	B3-U0-G5	
	Lumens per Watt	141	131	123	118	139	131	122	117	139	132	123	117	

5NQ	Lumens	19,636	24,078	29,802	32,692	24,201	29,677	36,731	40,294	28,992	35,552	44,003	48,270	
	BUG Rating	B4-U0-G2	B4-U0-G2	B5-U0-G2	B5-U0-G2	B4-U0-G2	B5-U0-G2	B5-U0-G3	B5-U0-G3	B4-U0-G2	B5-U0-G3	B5-U0-G3	B5-U0-G3	
	Lumens per Watt	152	141	132	127	149	141	132	126	150	143	132	126	

5MQ	Lumens	20,341	24,945	30,873	33,868	25,071	30,744	38,052	41,743	30,035	36,830	45,584	50,006	
	BUG Rating	B4-U0-G2	B5-U0-G3	B5-U0-G3	B5-U0-G4	B5-U0-G3	B5-U0-G3	B5-U0-G4	B5-U0-G4	B5-U0-G3	B5-U0-G4	B5-U0-G4	B5-U0-G4	
	Lumens per Watt	158	146	137	131	155	146	136	130	156	148	137	131	

5WQ	Lumens	19,872	24,368	30,161	33,086	24,493	30,035	37,174	40,780	29,341	35,980	44,532	48,852	
	BUG Rating	B5-U0-G3	B5-U0-G3	B5-U0-G4	B5-U0-G4	B5-U0-G3	B5-U0-G4	B5-U0-G4	B5-U0-G4	B5-U0-G4	B5-U0-G4	B5-U0-G5	B5-U0-G5	
	Lumens per Watt	154	143	134	128	151	143	133	127	152	144	134	128	

SLL/ SLR	Lumens	16,870	20,688	25,605	28,089	20,793	25,496	31,559	34,620	24,908	30,545	37,805	41,472	
	BUG Rating	B2-U0-G4	B3-U0-G4	B3-U0-G5	B3-U0-G5	B3-U0-G4	B3-U0-G5	B3-U0-G5	B3-U0-G5	B3-U0-G5	B3-U0-G5	B3-U0-G5	B3-U0-G5	
	Lumens per Watt	131	121	114	109	128	121	113	108	129	123	114	109	

RW	Lumens	19,519	23,935	29,625	32,498	24,057	29,500	36,512	40,054	28,818	35,340	43,739	47,982	
	BUG Rating	B4-U0-G2	B4-U0-G2	B5-U0-G3	B5-U0-G3	B4-U0-G2	B5-U0-G3	B5-U0-G3	B5-U0-G3	B5-U0-G3	B5-U0-G3	B5-U0-G4	B5-U0-G4	
	Lumens per Watt	151	140	132	126	149	140	131	125	149	142	131	126	

AFL	Lumens	19,571	24,000	29,705	32,586	24,121	29,578	36,611	40,162	28,896	35,434	43,858	48,112	
	BUG Rating	B2-U0-G2	B3-U0-G2	B3-U0-G3	B3-U0-G3	B3-U0-G2	B3-U0-G3	B3-U0-G3	B3-U0-G3	B3-U0-G3	B3-U0-G3	B3-U0-G3	B3-U0-G3	
	Lumens per Watt	152	140	132	126	149	141	131	126	150	142	132	126	
NOTES: 1. Photometric data published here for 740, 750, 760 Color Temperature options. For other options, refer to published IES files on product webpage or Supplemental Performance Tables.

Control Options
0-10V
This fixture provides 0-10V dimming wire leads for use with a lighting control panel or other control method.
Photocontrol (PR and PR7)
Photocontrol receptacles provide a flexible solution to enable "dusk-to-dawn" lighting by sensing light levels. Advanced control systems compatible with NEMA 7-PIN standards can be utilized with the PR7 receptacle.
After Hours Dim (AHD)
This feature allows photocontrol-enabled luminaires to achieve additional energy savings by dimming during scheduled portions of the night. The dimming profile will automatically take effect after a “dusk-to-dawn” period has been calculated from the photocontrol input. Specify the desired dimming profile for a simple, factory- shipped dimming solution requiring no external control wiring. Reference the After Hours Dim supplemental guide for additional information.
Dimming Occupancy Sensor (SPB, MS/DIM-LXX, MS/X-LXX and MS-LXX)
When a sensor for dimming operation (MS/DIM) option is selected, the luminaire will dim down to approximately 50 percent power after five mintues of no activity detected. When activity is detected, the luminaire returns to full light output. When a sensor for ON/OFF operation (MS-LXX) is selected, the luminaire will turn off after five minutes of no activity. When a sensor for bi-level operation (MS/X) is selected, the specified number of light engines will shut off after five minutes of inactivity. The remaining light engines will remain on. The SPB sensor is factory preset to dim down to approximately 10% power with a time delay of five minutes. The SPB requires the Sensor Configuration mobile application by Wattstopper or iOS and Android devices to change factory default dimming level, time delay, sensitivity and other parameters.
These occupancy sensors include an integral photocell that can be activated or inactivated with the programming remote / configuration tool for “dusk-to-dawn” control or daylight harvesting - the factory preset is OFF (Disabled.) The programming remote / tool is a wireless tool that can be utilized to change the dimming level, time delay, sensitivity and other parameters. A variety of sensor lenses are available to optimize the coverage pattern for mounting heights from 8’-40’.

For mounting heights up to 8' (SPB1, -L08)
0

For mounting heights up to 20' (SPB2, -L20)
0

8
12
36	24	18

7	5	0	5	7

5

18	24	36

Coverage Side Area (Feet)	10

For mounting heights up to 40' (SPB4, -L40W)
0

15

20
20  18  15  12	9	6	3	0	3	6

9	12  15  18  20

5	Coverage Side Area (Feet)

7

0
50	40

30	20	10	0

10	20	30

40	50

Coverage Side Area (Feet)

WaveLinx Wireless Control and Monitoring System Available in 7-PIN configurations, the WaveLinx Outdoor control platform operates on a wireless mesh network based on IEEE 802.15.4 standards enabling wireless control of outdoor lighting. Use the WaveLinx Mobile application for set-up and configuration. At least one Wireless Area Controller (WAC) is required for full functionality and remote communication (including adjustment of any factory pre-sets).
WaveLinx Outdoor Control Module (WOLC-7P-10A) A photocontrol that enables astronomic or time-based schedules to provide ON, OFF and dimming control of fixtures utilizing a 7-PIN receptacle. The out-of-box functionality is ON at dusk and OFF at dawn.

Enlighted Wireless Control and Monitoring System (LWR-LW and LWR-LN)
Enlighted is a connected lighting solution that combines LED luminaires with an integrated wireless sensor system. The sensor controls the lighting system in compliance with the latest energy codes and collects valuable data about building performance and use. Software applications turn the granular data into information through energy dashboards and specialized apps that make it simple and help optimize the use of building resources, beyond lighting.

For mounting heights from 8' to 16' (LWR-LW)	For mounting heights from 16' to 40' (LWR-LN)
0	0

20

30

16
24	8	18	0

40
8	18	24
Coverage Side Area (Feet)

40	30	20	10

0	10	20	30	40
Coverage Side Area (Feet)

LumenSafe (LD)
The LumenSafe integrated network camera is a streamlined, outdoor-ready camera that provides high definition video surveillance. This IP camera solution is optically designed to integrate into virtually any video management system or security software platform of choice. No additional wiring is needed beyond providing line voltage power to the luminaire. LumenSafe features factory-installed power and networking gear in a variety of networking options allowing security integrators to design the optimal solution for active surveillance.

Cooper Lighting Solutions 1121 Highway 74 South Peachtree City, GA 30269 P: 770-486-4800
www.cooperlighting.com

© 2022 Cooper Lighting Solutions All Rights Reserved.

Specifications and dimensions subject to change without notice.

PS521003EN page 7
July 15, 2022 7:18 PM

Tab 6

Heritage Landing CDD Meeting
December 14, 2023, 1:00 p.m.

Date of Report: December 6, 2023	Todd Myhill, Amenity Manager

	Upcoming Events: Pictures with Santa—No Board Action Required
Pictures with Santa with Flashback Photography. We will have an easy ornament
craft, cookies and hot chocolate, and a traditional “Letter to Santa” station complete with North Pole post mark. This event will be held over two days, December 15 and
16. Over 100 families have signed up so far, with plenty of room for more.	
	Amenity Athletics Calendar for 2024—Board Action Required
Please find the annual calendar for Amenity Athletics attached to this report for your review and approval.	
Chomic Combat Karate Program—Board Action Required
Nichola Chomic is requesting an agreement with the board to provide karate classes at the amenity center two days a week, two hours per class. Mr. Chomic’s proposal is
attached to this report.
Vector Security Repair or Upgrade—Board Action Required
The mother board for the building security system has failed, likely due to past elec- trical surge from lightning. Vector security has proposed to replace the board with a
separate communicator or provide an upgraded board with the communicator integrat- ed, either board with or without the ability to access via cell phone app. Please see the attached chart and a proposal letter from Vector.

SJMSS—No Board Action Required
SJMSS has withdrawn their request to use Heritage Landing’s tennis courts for this tennis season.
Facility Information—No Board Action Required
No facility items to report.

Marketing Begins October 1, 2023
Registration Begins: November 1, 2023
Registration CLOSED: December 15, 2023
Practice could begin as early as January 8, 2024
Season Games: January 20 – March 2, 2024
Heritage Landing Games: February 3, 17, 24
Picture Day: Bartram Springs, February 10, 2024
FREE Flag Football Workshop:
Bartram Springs: Saturday, December 9, 2023, 1:00-2:30pm

Spring Soccer Season 2024
Games played Saturdays at both Bartram Springs and Heritage Landing
Marketing Begins December 1, 2023
Registration Begins: January 1, 2024
Registration Ends: January 28, 2024
Late Registration with $45 late fee, One Week ONLY
January 29-February 5
Practice could begin as early as March 11
Season Games: March 23 - May 18, 2024
No games Easter Weekend; March 30
Picture Day: Bartram Springs- April 13, Heritage Landing- April 15, 16, 18

Basketball Season 2024
Games played Wednesday afternoons.
Marketing Begins February 1, 2024
Registration Begins: March 1, 2024
Registration Ends: March 31, 2024 (ONLY 1 Month)
Practice could begin as early as April 8, 2024
Season Games: April 24 - May 29, 2024
Picture Day May 8, 2024

Fall Soccer Season 2024
Games played Saturdays at both Bartram Springs and Heritage Landing
Marketing Begins June 1, 2024
Registration Begins: July 1, 2024
Registration Ends: July 28, 2024
Late Registration with $45 late fee, One Week ONLY
July 29 – August 4 ONLY
Practice could begin as early as September 2, 2024
Season Games: September 21 - November 9, 2024
Picture Day: Bartram Spring – 10/5, Heritage Landing – 10/14, 15, 17

Marketing Begins October 1, 2024
Registration Begins: November 1, 2024
Registration Ends: November 24, 2024
Late Registration with $45 late fee
November 25-30 ONLY
Practice could begin as early as January 6, 2025
Season Games: January 18 – March 1, 2025
Heritage Landing Games: February 1, 15, 22
Picture Day: Bartram Springs, February 8, 2025
FREE Flag Football Workshop:
Bartram Springs - Saturday, December 7, 2024, 10:00-12:00pm

November 30, 2023
Heritage Landing Supervisors,
Chomic Combat Karate (CCK) is traditional martial arts school that teaches the art of Tang Soo Do, with origins dating back over 2000 years. There is no doubt we all need self-defense skills. Equally important are physical fitness & methods for the release of daily stress – No matter whether you are seeking self-defense, better health, physical fitness or discipline, our CCK team can meet your needs. However, CCK has its own unique character which differentiates it from any other form of martial arts or martial sports. The real value of CCK is not the belt you earn, but the changes that occur within you, in your quest for them. These changes include the betterment of mind, body and spirit, also the development of individual character and respect for others. The other goal of CCK training is to use the lessons you learn in the studio to enrich every part of your life.

A little bit about us and what we offering:

Tuition: Tiny Tigers & Little Dragons Program (Ages 4-7): $165/month per student // we currently have: 7 students in this program
Gups Program (Ages +8): $175/month per student // we currently have: 23 students in this program Master Club (+9): $75/month add per member // we currently have: 3 students in this program

Art: Tang Soo Do (South Korean Karate)

We are apart of the World Tang Soo Do Association: https://worldtangsoodo.com Our School Name: Chomic Combat Karate: https://www.chomiccombatkarate.com Corporation: LLC - Detail by Entity Name (sunbiz.org)
Insurance: Small Business Insured by NEXT Insurance Attached a Copy of our COI with Heritage Landing
(added for our meeting)

Equipment: We will set up and teardown for all classes, clean our mess, if any, after every class (we will only leave footprints and memories behind), and we will provide all the equipment needed to teach classes.

Class Schedule: We currently have 30 students, to include 2 instructors fully trained (Black Belts), and 6 instructors in training (Blue Belts)

I currently work during the day (6:00am - 2:30pm) for the Department of Defence at	Navy Air Station JAX.

Current CCK Classes: Subject to change based on what Heritage Landing can provide.
Ages 4-7: 5:30pm - 6:00pm Mon - Thur

Ages +8 years: 6:00pm - 6:45pm (Beginner Class) Mon -Thur
Ages +8 years: 6:00pm - 6:45pm (Advance Class) Mon -Thur
Masters Club & Black Belt Class: 5:30pm - 7:30pm Every Friday

\\ SIGNED// Nicholas W. Chomic CEO/Chief Instructor

9456 Philips Hwy.
Suite 1
Jacksonville, FL 32256
www.vectorsecurity.com

Dear Heritage Landing C.D.D,

I hope this email finds you well. I was able to get more information from management regarding upgrading your system or just adding a cell communicator to your system. As well as the replacement panel.

Cell communicator - it is a device we will place in to take the place of the landline that will then communicate via the cell towers (Verizon or At&t).

Option 1: 1x fee of $299+ (19.44 tax) = $318.44 with an additional $15/month without contract

Option 2: No charge with an additional $20 with a new 3-year term (with the ability to arm and disarm system via phone or computer)

With the Cell Communicator option if you sign the 3-year term, we will come out and replace the panel at $199 + (14.93 tax) = $213.93 and we will waive the labor fee of
$115 plus tax. If you decide to do option 1 and not sign a 3-year term, we will replace the panel at $199 plus tax and there will be a labor fee of $115 plus tax.

We also have the option to upgrade the system that includes the cell communicator in the panel itself.

Qolsys Upgrade - wireless touchscreen security system to where a cell communicator is built in with the ability to arm and disarm system via phone or computer.

Option 1: No charge with a new 3-year term @ $49.95+tax without the ability to arm and disarm from phone or computer.

Option 2: No charge with a 3-year term @ $54.95+tax with the ability to arm and dis arm system.

Taylor Collins

Customer Service Representative Branch 72 Jacksonville.

ector Security is a registered trademark of Vector Security, Inc. Licenses: AK 09-017; AL AESBL 11-817, 44814; AR E 2005 0104; AZ ROC218982; CA ACO 6152, 914676; DE 1989004898; FL EF20000395, EF0001062, EF20000934, EF20000933, EF20000596; HI C 27082; LA 317, 54974; MA 1594 C; NC 2313-CSA; ND 37153; NJ , 13VH00292300, Fire Alarm, Burglar Alarm and Locksmith Business Lic. # 34AL00000400; NV F 437, 0066031; NY 12000234360; OH 53-50-1081; OK 559; PA PA004997; RI 30394, AFC-0449; TN 0444, 1341, 1551,
552; TX B11645; UT 4759383-6501; VA DCJS #11-2048; WA VECTOSI957PE; WV WV043469. Additional license information available at www.vectorsecurity.com.

Vector Security for Heritage Landing*--December 5, 2023

		Option 1	Option 2	Option 3	Option 4	Option 5	
	
Current Contract Monthly Fee	No Contract; Replace board; install external cell comm.	3-Year Contract; Replace board; install external
cell comm.	3-Year Contract; Replace board; install external
cell comm.	Qolsys Upgrade w/ built in comm. 3-Year Contract.	Qolsys Upgrade w/ built in comm. 3-Year Contract.	
							
Replace Panel	N/A	$199.00	$0.00	$199.00	$0.00	$0.00	
Install Cell
Communicator	N/A	$299.00	$0.00	$0.00	$0.00	$0.00	
Labor	N/A	$115.00	$0.00	$0.00	$0.00	$0.00	
Total Parts and
Labor	N/A	$613.00	$0.00	$199.00	$0.00	$0.00	
Monthly Fee	$25.73	$40.73	$45.73	$40.73	49.95	$54.95	
Arm/Disarm
with Cellphone	No	No	Yes	No	No	Yes	

Additional
Annual Cost		$180.00	$240.00	$180.00	$290.64	$350.64	
Parts and Labor		$613.00	$0.00	$199.00	$0.00	$0.00	

Options 1-3; install of panel and cell communicator would not be at the same time.

Tab 7

Heritage Landing CDD Meeting December 14, 2023
Field Operations Manager Report
Date of report: 12/5/2023

Tennis Courts:
Due to the resurfacing project starting only in next year we started pressure washing all the tennis courts. We should be finished by the end of December

Women’s Bathroom:
The finish on the bathroom doors are deteriorating and the handles are corroded. We removed the old bad handles, scrapped and sanded the stalls doors. We applied a wood finish that blended very good and new hardware will be installed.

Gym AC Thermostat:
Recently the gym AC stopped working. After some investigation it was found that the wire between the AC handler and the thermostat was bad. We were given a proposal for $900 to run new wire and conduit. At the same inspection they found the TXV valve was bad and the proposal to replace was
$790. I asked our vendor if my team could run the wire and conduit to save that money, in turn we will use that savings to have the TXV valve replaced. They were ok with that, I and Jeff ran an 18/8 shielded cable and the thermostat was wired up the same day the TXV was replaced. The AC is functioning properly again.

FPL Light Pole:
The light post on the corner of Heritage Landing Pkwy and Steamboat Landing was hit by an unknown vehicle on a Friday evening around 10:35pm. Our cameras picked up the incident but were unable to make a positive identification. The Saturday morning I was notified and I noticed that there was still live power to it. I contacted FPL to report it and they need to come disconnect the power to it. That was done on Saturday and I placed caution tape around it. The light was replaced the following week.

General Maintenance:

Making new trashcan lids from pvc and wood

Swing repairs

New tennis net installed

New sump pump installed in slide pump tomb

Replaced several uranals flush valves

Our office power back up system’s batteries failed
and I replaced them under warranty.

Lourens Erasmus
General Manager

370 Heritage Landing Pkwy Saint Augustine, FL 32092 P: 904.940.6095
C: 904.536.6217
www.VestaPropertyServices.com

Tab 8

	6869 Phillips Pkwy Dr. South Jacksonville Fl 32256	 Fax: 904-807-9158	Phone: 904-997-0044
Service Report
Date: November 9 & 21, 2023	Biologists: Jim Charles

Client: Heritage Landing CDD

Waterways: Thirteen Ponds

Comments: Sunny on the 9th, 72° F and calm.

Pond 1: Pond was in good condition. The water level is good. Minor spatterdock noted.

Pond 2: Pond was in fair to good condition. The water level is normal. Fountain running. Treated perimeter for torpedo grass.

Pond 3: Pond was in good condition. The water level is good. Treated perimeter for torpedo grass and Cogan grass on shoreline.

Pond 4: Pond was in fair condition. Both fountains are running. Treated perimeter for torpedo grass and spatterdock. Added four more gallons of pond dye as previous application was ineffective (no charge).

Pond 5: Pond was in fair condition. The water level is normal. Treated for algae.

Pond 6: Pond was in fair condition. The water level is normal. Treated perimeter for spike rush.

Pond 7: Pond was in fair to good condition. The water level is good. Treated minor algae along perimeter.

Pond 8: Pond was in good condition. The water level is normal. Fountain running.

Pond 9: Pond was in good condition. The water level is good.

Pond 10: Pond was in good condition. The water level is good. Minor spatter dock noted.

Pond 11: Pond was in very good condition this month. The water level is normal.

Pond 12: Pond was in good condition. The water level is normal.

Pond 13: Pond was in good condition. The water level is normal. Added four more gallons of pond dye to this pond also on the 9th. Pond color looks much better on the 21st.

Jim Charles